chip northbridge/amd/amdk8/root_complex		# Root complex
  device lapic_cluster 0 on			# APIC cluster
    chip cpu/amd/socket_754			# Socket 754 CPU
      device lapic 0 on end			# APIC
    end
  end

  device pci_domain 0 on			# PCI domain
    chip northbridge/amd/amdk8			# mc0
      device pci 18.0 on			# Northbridge
        # Devices on link 0, link 0 == LDT 0
        chip southbridge/nvidia/ck804		# Southbridge
          device pci 0.0 on end			# HT
          device pci 1.0 on			# LPC
            chip superio/winbond/w83627thf	# Super I/O
              device pnp 4e.0 on		# Floppy
                io 0x60 = 0x3f0
                irq 0x70 = 6
                drq 0x74 = 2
              end
              device pnp 4e.1 on		# Parallel port
                io 0x60 = 0x378
                irq 0x70 = 7
                drq 0x74 = 3
              end
              device pnp 4e.2 on		# Com1
                io 0x60 = 0x3f8
                irq 0x70 = 4
              end
              device pnp 4e.3 on		# Com2
                io 0x60 = 0x2f8
                irq 0x70 = 3
              end
              device pnp 4e.5 on		# PS/2 keyboard
                io 0x60 = 0x60
                io 0x62 = 0x64
                irq 0x70 = 1
                irq 0x72 = 12
              end
              device pnp 4e.6 off end		# XXX keep allocator happy
              device pnp 4e.7 off end		# Game, MIDI, GPIO 1, GPIO 5
              device pnp 4e.8 off end		# GPIO 2
              device pnp 4e.9 off end		# GPIO 3, GPIO 4
              device pnp 4e.a off end		# ACPI
              device pnp 4e.b on		# Hardware monitor
                io 0x60 = 0x290
                irq 0x70 = 5
              end
            end
          end
          device pci 1.1 on end			# SMbus
          device pci 2.0 on end			# USB 1.1
          device pci 2.1 on end			# USB 2
          device pci 4.0 on end			# Onboard audio (ACI)
          device pci 4.1 off end		# Onboard modem (MCI) -- not wired out
          device pci 6.0 on end			# IDE
          device pci 7.0 on end			# SATA 1
          device pci 8.0 on end			# SATA 0
          device pci 9.0 on end			# PCI
          device pci a.0 on end			# NIC
          device pci b.0 off end		# PCI E 3 -- not wired out
          device pci c.0 off end		# PCI E 2 -- not wired out
          device pci d.0 on end			# PCI E 1
          device pci e.0 on end			# PCI E 0
          register "ide0_enable" = "1"
          register "ide1_enable" = "1"
          register "sata0_enable" = "1"
          register "sata1_enable" = "1"
        end
      end
      device pci 18.1 on end
      device pci 18.2 on end
      device pci 18.3 on end
    end
  end
end
