chip northbridge/amd/amdk8/root_complex		# Root complex
  device lapic_cluster 0 on			# APIC cluster
    chip cpu/amd/socket_AM2			# CPU
      device lapic 0 on end			# APIC
    end
  end
  device pci_domain 0 on			# PCI domain
    chip northbridge/amd/amdk8			# Northbridge / mc0
      device pci 18.0 on
        # Devices on link 0, link 0 == LDT 0
        chip southbridge/nvidia/mcp55		# Southbridge
          device pci 0.0 on end			# HT
          device pci 1.0 on			# LPC
            chip superio/winbond/w83627ehg	# Super I/O
              device pnp 4e.0 on		# Floppy
                io 0x60 = 0x3f0
                irq 0x70 = 6
                drq 0x74 = 2
              end
              device pnp 4e.1 on		# Parallel port
                io 0x60 = 0x378
                irq 0x70 = 7
              end
              device pnp 4e.2 on		# Com1
                io 0x60 = 0x3f8
                irq 0x70 = 4
              end
              device pnp 4e.3 on		# Com2 / IrDA
                io 0x60 = 0x2f8
                irq 0x70 = 3
              end
              device pnp 4e.5 on		# PS/2 keyboard
                io 0x60 = 0x60
                io 0x62 = 0x64
                irq 0x70 = 1			# PS/2 keyboard IRQ
                irq 0x72 = 12			# PS/2 mouse IRQ
              end
              device pnp 4e.6 off		# Serial flash interface
                # io 0x62 = 0x100
              end
              device pnp 4e.7 off		# GPIO1/6, game port, MIDI port
                # io 0x60 = 0x220		# Datasheet: 0x201
                # io 0x62 = 0x300		# Datasheet: 0x330
                # irq 0x70 = 9
              end
              device pnp 4e.8 off		# WDTO#, PLED
              end
              device pnp 4e.9 off		# GPIO2/3/4/5, SUSLED
              end
              device pnp 4e.a off		# ACPI
              end
              device pnp 4e.b on		# HWM (for lm-sensors)
                io 0x60 = 0xa10
              end
            end
          end
          device pci 1.1 on			# SM 0
            chip drivers/generic/generic	# DIMM 0-0-0
              device i2c 50 on end
            end
            chip drivers/generic/generic	# DIMM 0-0-1
              device i2c 51 on end
            end
            chip drivers/generic/generic	# DIMM 0-1-0
              device i2c 52 on end
            end
            chip drivers/generic/generic	# DIMM 0-1-1
              device i2c 53 on end
            end
            # TODO: Needed?
            # chip drivers/generic/generic	# DIMM 1-0-0
            #   device i2c 54 on end
            # end
            # chip drivers/generic/generic	# DIMM 1-0-1
            #   device i2c 55 on end
            # end
            # chip drivers/generic/generic	# DIMM 1-1-0
            #   device i2c 56 on end
            # end
            # chip drivers/generic/generic	# DIMM 1-1-1
            #   device i2c 57 on end
            # end
          end
          # TODO: Check if the stuff below is correct / needed.
          device pci 1.1 on			# SM 1
            # PCI device SMBus address will depend on addon PCI device,
            # do we need to scan_smbus_bus?

            # chip drivers/generic/generic	# PCIXA Slot1
            #   device i2c 50 on end
            # end
            # chip drivers/generic/generic	# PCIXB Slot1
            #   device i2c 51 on end
            # end
            # chip drivers/generic/generic	# PCIXB Slot2
            #   device i2c 52 on end
            # end
            # chip drivers/generic/generic	# PCI Slot1
            #   device i2c 53 on end
            # end
            # chip drivers/generic/generic	# Master MCP55 PCI-E
            #   device i2c 54 on end
            # end
            # chip drivers/generic/generic	# Slave MCP55 PCI-E
            #   device i2c 55 on end
            # end
            chip drivers/generic/generic	# MAC EEPROM
              device i2c 51 on end
            end
          end
          device pci 2.0 on end			# USB 1.1
          device pci 2.1 on end			# USB 2
          device pci 4.0 on end			# IDE
          device pci 5.0 on end			# SATA 0
          device pci 5.1 on end			# SATA 1
          device pci 5.2 off end		# SATA 2 (N/A on this board)
          device pci 6.0 on end			# PCI
          device pci 6.1 on end			# AZA (HD Audio)
          device pci 8.0 on end			# NIC
          device pci 9.0 off end		# NIC (N/A on this board)
          device pci a.0 off end		# PCI E 5 (N/A on this board?)
          device pci b.0 on end			# PCI E 4
          device pci c.0 on end			# PCI E 3
          device pci d.0 on end			# PCI E 2
          device pci e.0 on end			# PCI E 1
          device pci f.0 on end			# PCI E 0
          register "ide0_enable" = "1"
          register "sata0_enable" = "1"
          register "sata1_enable" = "1"
          # TODO: Check the two lines below.
          register "mac_eeprom_smbus" = "3"	# 1: SMBus under 2e.8, 2: SM0 3: SM1
          register "mac_eeprom_addr" = "0x51"
        end
      end
      device pci 18.0 on end			# Link 1
      device pci 18.0 on end
      device pci 18.1 on end
      device pci 18.2 on end
      device pci 18.3 on end
    end
  end

# TODO
#  chip drivers/generic/debug
#    device pnp 0.0 off end			# chip name
#    device pnp 0.1 on end			# pci_regs_all
#    device pnp 0.2 on end			# mem
#    device pnp 0.3 off end			# cpuid
#    device pnp 0.4 on end			# smbus_regs_all
#    device pnp 0.5 off end			# dual core msr
#    device pnp 0.6 off end			# cache size
#    device pnp 0.7 off end			# tsc
#    device pnp 0.8 off end			# io
#    device pnp 0.9 off end			# io
#  end

end
