chip northbridge/intel/i855
	device pci_domain 0 on
		device pci 0.0 on end
		device pci 1.0 on end
		chip southbridge/intel/i82801dx
#			pci 11.0 on end
#			pci 11.1 on end
#			pci 11.2 on end
#			pci 11.3 on end
#			pci 11.4 on end
#			pci 11.5 on end
#			pci 11.6 on end
#			pci 12.0 on end
			register "enable_usb" = "0"
			register "enable_native_ide" = "0"
			chip superio/winbond/w83627hf # link 1
                	        device pnp 2e.0 on      #  Floppy
                	                 io 0x60 = 0x3f0
                	                irq 0x70 = 6
                	                drq 0x74 = 2
				end
                	        device pnp 2e.1 off     #  Parallel Port
                	                 io 0x60 = 0x378
                	                irq 0x70 = 7
				end
                	        device pnp 2e.2 on      #  Com1
                	                 io 0x60 = 0x3f8
                	                irq 0x70 = 4
				end
                	        device pnp 2e.3 off     #  Com2
                	                io 0x60 = 0x2f8
                	                irq 0x70 = 3
				end
                	        device pnp 2e.5 on      #  Keyboard
                	                 io 0x60 = 0x60
                	                 io 0x62 = 0x64
                	                irq 0x70 = 1
					irq 0x72 = 12
				end
                	        device pnp 2e.6 off end #  CIR
                	        device pnp 2e.7 off end #  GAME_MIDI_GIPO1
                	        device pnp 2e.8 off end #  GPIO2
                	        device pnp 2e.9 off end #  GPIO3
                	        device pnp 2e.a off end #  ACPI
                	        device pnp 2e.b on      #  HW Monitor
 					 io 0x60 = 0x290
				end
				register "com1" = "{1}"
			#	register "com1" = "{1, 0, 0x3f8, 4}"
			#	register "lpt" = "{1}"
                	end
		end
	end
	device lapic_cluster 0 on
		chip cpu/intel/socket_mPGA479M
			device lapic 0 on end
		end
	end
end
