chip northbridge/amd/amdk8/root_complex
        device lapic_cluster 0 on
                chip cpu/amd/socket_940
                        device lapic 0 on end
                end
        end
	device pci_domain 0 on
		chip northbridge/amd/amdk8
			device pci 18.0 on #  northbridge
				#  devices on link 0, link 0 == LDT 0
				chip southbridge/amd/amd8151
					# the on/off keyword is mandatory
					device pci 0.0 on end
					device pci 1.0 on end
				end
				chip southbridge/amd/amd8111
					# this "device pci 0.0" is the parent the next one
					# PCI bridge
					device pci 0.0 on
						device pci 0.0 on end
						device pci 0.1 on end
						device pci 0.2 off end
						device pci 1.0 off end
                                                device pci 5.0 on end
					end
					device pci 1.0 on
						chip superio/winbond/w83627hf
							device pnp 2e.0 on #  Floppy
								io 0x60 = 0x3f0
								irq 0x70 = 6
								drq 0x74 = 2
							end
							device pnp 2e.1 off #  Parallel Port
								io 0x60 = 0x378
								irq 0x70 = 7
							end
							device pnp 2e.2 on #  Com1
								io 0x60 = 0x3f8
								irq 0x70 = 4
							end
							device pnp 2e.3 off #  Com2
								io 0x60 = 0x2f8
								irq 0x70 = 3
							end
							device pnp 2e.5 on #  Keyboard
								io 0x60 = 0x60
								io 0x62 = 0x64
								irq 0x70 = 1
								irq 0x72 = 12
							end
							device pnp 2e.6 off #  CIR
								io 0x60 = 0x100
							end
							device pnp 2e.7 off #  GAME_MIDI_GIPO1
								io 0x60 = 0x220
								io 0x62 = 0x300
								irq 0x70 = 9
							end
							device pnp 2e.8 off end #  GPIO2
							device pnp 2e.9 off end #  GPIO3
							device pnp 2e.a off end #  ACPI
							device pnp 2e.b on #  HW Monitor
								io 0x60 = 0x290
								irq 0x70 = 5
							end
						end
					end
					device pci 1.1 on end
					device pci 1.2 on end
					device pci 1.3 on end
					device pci 1.5 on end
					device pci 1.6 off end
                                        register "ide0_enable" = "1"
                                        register "ide1_enable" = "1"
				end
			end #  device pci 18.0

			device pci 18.0 on end
			device pci 18.0 on end

			device pci 18.1 on end
			device pci 18.2 on end
			device pci 18.3 on end
		end
	end
end

