chip northbridge/intel/i82810			# Northbridge
  device lapic_cluster 0 on			# APIC cluster
    chip cpu/intel/socket_PGA370		# CPU
      device lapic 0 on end			# APIC
    end
  end
  device pci_domain 0 on
    device pci 0.0 on end			# Host bridge
    device pci 1.0 off end			# Onboard video
    chip southbridge/intel/i82801ax		# Southbridge
      register "ide0_enable" = "1"
      register "ide1_enable" = "1"

      device pci 1e.0 on end			# PCI bridge
      device pci 1f.0 on			# ISA/LPC bridge
        chip superio/smsc/smscsuperio		# Super I/O (SMSC LPC47B27x)
          device pnp 2e.0 on			# Floppy
            io 0x60 = 0x3f0
            irq 0x70 = 6
            drq 0x74 = 2
          end
          device pnp 2e.3 on			# Parallel port
            io 0x60 = 0x378
            irq 0x70 = 7
            drq 0x74 = 3
          end
          device pnp 2e.4 on			# Com1
            io 0x60 = 0x3f8
            irq 0x70 = 4
          end
          device pnp 2e.5 off end		# Com2 (N/A)
          device pnp 2e.7 on			# PS/2 keyboard
            irq 0x70 = 1
            irq 0x72 = 0
          end
          device pnp 2e.9 off end		# Game port (N/A)
          device pnp 2e.a on			# Power-management events (PME)
            io 0x60 = 0x800
          end
          device pnp 2e.b on			# MIDI port
            io 0x60 = 0x330
            irq 0x70 = 5
          end
        end
      end
      device pci 1f.1 on end			# IDE
      device pci 1f.2 on end			# USB
      device pci 1f.3 on end			# SMBus
      device pci 1f.5 on end			# AC'97 audio
      device pci 1f.6 off end			# AC'97 modem (N/A)
    end
  end
end

