chip northbridge/amd/amdk8/root_complex
	device lapic_cluster 0 on
		chip cpu/amd/socket_940
			device lapic 0 on end
		end
	end
	device pci_domain 0 on
		chip northbridge/amd/amdk8 #mc0
			device pci 18.0 on #  northbridge
				#  devices on link 0, link 0 == LDT 0
				chip southbridge/nvidia/ck804
					device pci 0.0 on end   # HT
					device pci 1.0 on # LPC
						chip superio/winbond/w83627hf
							device pnp 2e.0 off #  Floppy
								io 0x60 = 0x3f0
								irq 0x70 = 6
								drq 0x74 = 2
							end
							device pnp 2e.1 off #  Parallel Port
								io 0x60 = 0x378
								irq 0x70 = 7
							end
							device pnp 2e.2 on #  Com1
								io 0x60 = 0x3f8
								irq 0x70 = 4
							end
							device pnp 2e.3 off #  Com2
								io 0x60 = 0x2f8
								irq 0x70 = 3
							end
							device pnp 2e.5 on #  Keyboard
								io 0x60 = 0x60
								io 0x62 = 0x64
								irq 0x70 = 1
								irq 0x72 = 12
							end
							device pnp 2e.6 off #  CIR
								io 0x60 = 0x100
							end
							device pnp 2e.7 off #  GAME_MIDI_GIPO1
								io 0x60 = 0x220
								io 0x62 = 0x300
								irq 0x70 = 9
							end
							device pnp 2e.8 off end #  GPIO2
							device pnp 2e.9 off end #  GPIO3
							device pnp 2e.a off end #  ACPI
							device pnp 2e.b off #  HW Monitor
								io 0x60 = 0x290
								irq 0x70 = 5
							end
						end
					end
					device pci 1.1 on # SM 0
#						chip drivers/generic/generic #dimm 0-0-0
#							device i2c 50 on end
#						end
#						chip drivers/generic/generic #dimm 0-0-1
#							device i2c 51 on end
#						end
#						chip drivers/generic/generic #dimm 0-1-0
#							device i2c 52 on end
#						end
#						chip drivers/generic/generic #dimm 0-1-1
#							device i2c 53 on end
#						end
#						chip drivers/generic/generic #dimm 1-0-0
#							device i2c 54 on end
#						end
#						chip drivers/generic/generic #dimm 1-0-1
#							device i2c 55 on end
#						end
#						chip drivers/generic/generic #dimm 1-1-0
#							device i2c 56 on end
#						end
#						chip drivers/generic/generic #dimm 1-1-1
#							device i2c 57 on end
#						end
					end # SM
#					device pci 1.1 on # SM 1
#						chip drivers/i2c/adm1027 # ADT7463A CPU0 temp, SYS FAN 2/3/4
#							device i2c 2d on end
#						end
#						chip drivers/i2c/adm1027 # ADT7463A CPU1 temp, CPU0/1 FAN , SYS FAN 1/5
#							device i2c 2e on end
#						end
#						chip drivers/generic/generic # Winbond HWM 0x54 CPU0/1 VRM temp, SYSFAN 6/7, SB FAN
#							device i2c 2a on end
#						end
#						chip drivers/generic/generic # Winbond HWM 0x92
#							device i2c 49 on end
#						end
#						chip drivers/generic/generic # Winbond HWM 0x94
#							device i2c 4a on end
#						end
#					end #SM
					device pci 2.0 on end # USB 1.1
					device pci 2.1 on end # USB 2
					device pci 4.0 off end # ACI
					device pci 4.1 off end # MCI
					device pci 6.0 on end # IDE
					device pci 7.0 on end # SATA 1
					device pci 8.0 on end # SATA 0
					device pci 9.0 on  # PCI
					#	chip drivers/ati/ragexl
						device pci 7.0 on end
					end
					device pci a.0 off end # NIC
					device pci b.0 off end # PCI E 3
					device pci c.0 off end # PCI E 2
					device pci d.0 on end # PCI E 1
					device pci e.0 on end # PCI E 0
					register "ide0_enable" = "1"
					register "ide1_enable" = "1"
					register "sata0_enable" = "1"
					register "sata1_enable" = "1"
				end
			end #  device pci 18.0
			device pci 18.0 on end # Link 1
			device pci 18.0 on
			#  devices on link 2, link 2 == LDT 2
				chip southbridge/amd/amd8131
					# the on/off keyword is mandatory
					device pci 0.0 on end
					device pci 0.1 on end
					device pci 1.0 on
						device pci 9.0 on end
						device pci 9.1 on end
					end
					device pci 1.1 on end
				end
			end # device pci 18.0
			device pci 18.1 on end
			device pci 18.2 on end
			device pci 18.3 on end
		end #mc0

	end # pci_domain

#	chip drivers/generic/debug
#		device pnp 0.0 off end # chip name
#		device pnp 0.1 off end # pci_regs_all
#		device pnp 0.2 off end # mem
#		device pnp 0.3 off end # cpuid
#		device pnp 0.4 off end # smbus_regs_all
#		device pnp 0.5 off end # dual core msr
#		device pnp 0.6 off end # cache size
#		device pnp 0.7 off end # tsc
#		device pnp 0.8 on  end # hard_reset
#	end
end # root_complex
