chip northbridge/amd/amdk8/root_complex
	device lapic_cluster 0 on
		chip cpu/amd/socket_940
			device lapic 0 on end
		end
	end
	device pci_domain 0 on
		chip northbridge/amd/amdk8
			device pci 18.0 on # LDT 0
				chip southbridge/amd/amd8131
					device pci 0.0 on end
					device pci 0.1 on end
					device pci 1.0 on end
					device pci 1.1 on end
				end
				chip southbridge/amd/amd8111
					# this "device pci 0.0" is the parent the next one
					# PCI bridge
					device pci 0.0 on
						device pci 0.0 on end
						device pci 0.1 on end
						device pci 0.2 on end
						device pci 1.0 off end
					end
					device pci 1.0 on
						chip superio/winbond/w83627hf
							device pnp  2e.0 on      # Floppy
								 io 0x60 = 0x3f0
								irq 0x70 = 6
								drq 0x74 = 2
							end
							device pnp  2e.1 off     # Parallel Port
								 io 0x60 = 0x378
								irq 0x70 = 7
							end
							device pnp  2e.2 on      # Com1
								 io 0x60 = 0x3f8
								irq 0x70 = 4
							end
							device pnp  2e.3 off     # Com2
								io 0x60 = 0x2f8
								irq 0x70 = 3
							end
							device pnp  2e.5 on      # Keyboard
								 io 0x60 = 0x60
								 io 0x62 = 0x64
							       irq 0x70 = 1
								irq 0x72 = 12
							end
							device pnp  2e.6 off end # CIR
							device pnp  2e.7 off end # GAME_MIDI_GIPO1
							device pnp  2e.8 off end # GPIO2
							device pnp  2e.9 off end # GPIO3
							device pnp  2e.a off end # ACPI
							device pnp  2e.b on      # HW Monitor
								 io 0x60 = 0x290
							end
							register "com1" = "{1}"
						#	register "com1" = "{1, 0, 0x3f8, 4}"
						#	register "lpt" = "{1}"
						end
					end
					device pci 1.1 on end
					device pci 1.2 on end
					device pci 1.3 on end
					device pci 1.5 off end
					device pci 1.6 off end
				end
			end # LDT0
			device pci 18.0 on end # LDT1
			device pci 18.0 on end # LDT2
			device pci 18.1 on end
			device pci 18.2 on end
			device pci 18.3 on end
		end
	end
end

