chip cpu/amd/sc520
	device pci_domain 0 on
		device pci 0.0 on end
		device pci 12.0 on end # enet
		device pci 14.0 on end # 69000
#		register "com1" = "{1}"
#		register "com1" = "{1, 0, 0x3f8, 4}"
	end

end
