chip northbridge/amd/amdk8/root_complex
  device lapic_cluster 0 on
    chip cpu/amd/socket_940
      device lapic 0 on end
    end
  end
  device pci_domain 0 on
    chip northbridge/amd/amdk8
      device pci 18.0 on end # link 0
      device pci 18.0 on end # link 1
      device pci 18.0 on     # link 2
        chip southbridge/amd/amd8131
          # the on/off keyword is mandatory
          device pci 0.0 on
            device pci 9.0 on end # Broadcom 5704
            device pci 9.1 on end
            device pci a.0 on end # Adaptic
            device pci a.1 on end
          end
          device pci 0.1 on end
          device pci 1.0 on end
          device pci 1.1 on end
        end
        chip southbridge/amd/amd8111
          # this "device pci 0.0" is the parent the next one
          # PCI bridge
          device pci 0.0 on
            device pci 0.0 on end
            device pci 0.1 on end
            device pci 0.2 off end
            device pci 1.0 off end
            device pci 5.0 on end # SiI
            device pci 6.0 on end
          end
          device pci 1.0 on
            chip superio/winbond/w83627hf
              device pnp 2e.0 on  # Floppy
                io  0x60 = 0x3f0
                irq 0x70 = 6
                drq 0x74 = 2
              end
              device pnp 2e.1 off # Parallel Port
                io  0x60 = 0x378
                irq 0x70 = 7
              end
              device pnp 2e.2 on  # Com1
                io  0x60 = 0x3f8
                irq 0x70 = 4
              end
              device pnp 2e.3 off # Com2
                io  0x60 = 0x2f8
                irq 0x70 = 3
              end
              device pnp 2e.5 on  # Keyboard
                io  0x60 = 0x60
                io  0x62 = 0x64
                irq 0x70 = 1
                irq 0x72 = 12
              end
              device pnp 2e.6 off # CIR
                io  0x60 = 0x100
              end
              device pnp 2e.7 off # GAME_MIDI_GIPO1
                io  0x60 = 0x220
                io  0x62 = 0x300
                irq 0x70 = 9
              end
              device pnp 2e.8 off end # GPIO2
              device pnp 2e.9 off end # GPIO3
              device pnp 2e.a off end # ACPI
              device pnp 2e.b on      # HW Monitor
                io  0x60 = 0x290
                irq 0x70 = 5
              end
            end
          end
          device pci 1.1 on end
          device pci 1.2 on end
          device pci 1.3 on
            chip drivers/generic/generic #dimm 0-0-0
              device i2c 50 on end
            end
            chip drivers/generic/generic #dimm 0-0-1
              device i2c 51 on end
            end
            chip drivers/generic/generic #dimm 0-1-0
              device i2c 52 on end
            end
            chip drivers/generic/generic #dimm 0-1-1
              device i2c 53 on end
            end
            chip drivers/generic/generic #dimm 1-0-0
              device i2c 54 on end
            end
            chip drivers/generic/generic #dimm 1-0-1
              device i2c 55 on end
            end
            chip drivers/generic/generic #dimm 1-1-0
              device i2c 56 on end
            end
            chip drivers/generic/generic #dimm 1-1-1
              device i2c 57 on end
            end
            chip drivers/i2c/adt7463 # CPU0/1 temp, CPU1 vid, SYS FAN 1/2/3
              device i2c 2d on end
            end
            chip drivers/generic/generic # Winbond HWM 0x54 CPU0/1 VRM temp, SYSFAN 4,CPU0 vid, CPU0/1 FAN
              device i2c 2a on end
            end
            chip drivers/generic/generic # Winbond HWM 0x92
              device i2c 49 on end
            end
            chip drivers/generic/generic # Winbond HWM 0x94
              device i2c 4a on end
            end
          end # acpi
          device pci 1.5 off end
          device pci 1.6 off end
          register "ide0_enable" = "1"
          register "ide1_enable" = "1"
        end
      end #  device pci 18.0
      device pci 18.1 on end
      device pci 18.2 on end
      device pci 18.3 on end
    end
  end
end

