/*
 * Copyright 2005 AMD
 */
//AMD8111 isa

            Device (ISA)
            {
                /* lpc  0x00040000 */
                Method (_ADR, 0, NotSerialized)
                {
			Return (DADD(\_SB.PCI0.SBDN, 0x00010000))
                }

                OperationRegion (PIRY, PCI_Config, 0x51, 0x02) // LPC Decode Registers
                Field (PIRY, ByteAcc, NoLock, Preserve)
                {
                    Z000,   2,  // Parallel Port Range
                        ,   1,
                    ECP,    1,  // ECP Enable
                    FDC1,   1,  // Floppy Drive Controller 1
                    FDC2,   1,  // Floppy Drive Controller 2
                    Offset (0x01),
                    Z001,   3,  // Serial Port A Range
                    SAEN,   1,  // Serial Post A Enabled
                    Z002,   3,  // Serial Port B Range
                    SBEN,   1  // Serial Post B Enabled
                }

                Device (PIC)
                {
                    Name (_HID, EisaId ("PNP0000"))
                    Name (_CRS, ResourceTemplate ()
                    {
                        IO (Decode16, 0x0020, 0x0020, 0x01, 0x02)
                        IO (Decode16, 0x00A0, 0x00A0, 0x01, 0x02)
                        IRQ (Edge, ActiveHigh, Exclusive) {2}
                    })
                }

                Device (DMA1)
                {
                    Name (_HID, EisaId ("PNP0200"))
                    Name (_CRS, ResourceTemplate ()
                    {
                        IO (Decode16, 0x0000, 0x0000, 0x01, 0x10)
                        IO (Decode16, 0x0080, 0x0080, 0x01, 0x10)
                        IO (Decode16, 0x00C0, 0x00C0, 0x01, 0x20)
                        DMA (Compatibility, NotBusMaster, Transfer16) {4}
                    })
                }

                Device (TMR)
                {
                    Name (_HID, EisaId ("PNP0100"))
                    Name (_CRS, ResourceTemplate ()
                    {
                        IO (Decode16, 0x0040, 0x0040, 0x01, 0x04)
                        IRQ (Edge, ActiveHigh, Exclusive) {0}
                    })
                }

                Device (RTC)
                {
                    Name (_HID, EisaId ("PNP0B00"))
                    Name (_CRS, ResourceTemplate ()
                    {
                        IO (Decode16, 0x0070, 0x0070, 0x01, 0x06)
                        IRQ (Edge, ActiveHigh, Exclusive) {8}
                    })
                }

                Device (SPKR)
                {
                    Name (_HID, EisaId ("PNP0800"))
                    Name (_CRS, ResourceTemplate ()
                    {
                        IO (Decode16, 0x0061, 0x0061, 0x01, 0x01)
                    })
                }

                Device (COPR)
                {
                    Name (_HID, EisaId ("PNP0C04"))
                    Name (_CRS, ResourceTemplate ()
                    {
                        IO (Decode16, 0x00F0, 0x00F0, 0x01, 0x10)
                        IRQ (Edge, ActiveHigh, Exclusive) {13}
                    })
                }

                Device (SYSR)
                {
                    Name (_HID, EisaId ("PNP0C02"))
                    Name (_UID, 0x00)
                    Name (SYR1, ResourceTemplate ()
                    {
                        IO (Decode16, 0x04D0, 0x04D0, 0x01, 0x02) //wrh092302 - added to report Thor NVRAM
                        IO (Decode16, 0x1100, 0x117F, 0x01, 0x80) //wrh092302 - added to report Thor NVRAM
                        IO (Decode16, 0x1180, 0x11FF, 0x01, 0x80)
                        IO (Decode16, 0x0010, 0x0010, 0x01, 0x10)
                        IO (Decode16, 0x0022, 0x0022, 0x01, 0x1E)
                        IO (Decode16, 0x0044, 0x0044, 0x01, 0x1C)
                        IO (Decode16, 0x0062, 0x0062, 0x01, 0x02)
                        IO (Decode16, 0x0065, 0x0065, 0x01, 0x0B)
                        IO (Decode16, 0x0076, 0x0076, 0x01, 0x0A)
                        IO (Decode16, 0x0090, 0x0090, 0x01, 0x10)
                        IO (Decode16, 0x00A2, 0x00A2, 0x01, 0x1E)
                        IO (Decode16, 0x00E0, 0x00E0, 0x01, 0x10)
                        IO (Decode16, 0x0B78, 0x0B78, 0x01, 0x04) // Added this to remove ACPI Unrepoted IO Error
                        IO (Decode16, 0x0190, 0x0190, 0x01, 0x04) // Added this to remove ACPI Unrepoted IO Error
                    })
                    Method (_CRS, 0, NotSerialized)
                    {
                        Return (SYR1)
                    }
                }

                Device (MEM)
                {
                    Name (_HID, EisaId ("PNP0C02"))
                    Name (_UID, 0x01)
                    Method (_CRS, 0, NotSerialized)
                    {
                        Name (BUF0, ResourceTemplate ()
                        {
                            Memory32Fixed (ReadWrite, 0x000E0000, 0x00020000) // BIOS E4000-FFFFF
                            Memory32Fixed (ReadWrite, 0x000C0000, 0x00010000) // video BIOS c0000-c8404
                            Memory32Fixed (ReadWrite, 0xFEC00000, 0x00001000) // I/O APIC
                            Memory32Fixed (ReadWrite, 0xFFC00000, 0x00380000) // LPC forwarded, 4 MB w/ROM
                            Memory32Fixed (ReadWrite, 0xFEE00000, 0x00001000) // Local APIC
                            Memory32Fixed (ReadWrite, 0xFFF80000, 0x00080000) // Overlay BIOS
                            Memory32Fixed (ReadWrite, 0x00000000, 0x00000000) // Overlay BIOS
                            Memory32Fixed (ReadWrite, 0x00000000, 0x00000000) // Overlay BIOS
                            Memory32Fixed (ReadWrite, 0x00000000, 0x00000000) //Overlay BIOS
                            Memory32Fixed (ReadWrite, 0x00000000, 0x00000000) //Overlay BIOS
                        })
			// Read the Video Memory length
                        CreateDWordField (BUF0, 0x14, CLEN)
                        CreateDWordField (BUF0, 0x10, CBAS)

                        ShiftLeft (VGA1, 0x09, Local0)
                        Store (Local0, CLEN)

                        Return (BUF0)
                    }
                }

                Device (PS2M)
                {
                    Name (_HID, EisaId ("PNP0F13"))
                    Name (_CRS, ResourceTemplate ()
                    {
                        IRQNoFlags () {12}
                    })
                    Method (_STA, 0, NotSerialized)
                    {
                        And (FLG0, 0x04, Local0)
                        If (LEqual (Local0, 0x04)) { Return (0x0F) }
                        Else { Return (0x00) }
                    }
                }

                Device (PS2K)
                {
                    Name (_HID, EisaId ("PNP0303"))
                    Name (_CRS, ResourceTemplate ()
                    {
                        IO (Decode16, 0x0060, 0x0060, 0x01, 0x01)
                        IO (Decode16, 0x0064, 0x0064, 0x01, 0x01)
                        IRQNoFlags () {1}
                    })
                }
		#include "superio.asl"

            }

