chip northbridge/intel/i82830		# Northbridge
  device lapic_cluster 0 on		# APIC cluster
    chip cpu/intel/socket_mFCBGA479	# Low Voltage PIII Micro-FCBGA Socket 479
      device lapic 0 on end		# APIC
    end
  end

  device pci_domain 0 on		# PCI domain
    device pci 0.0 on end		# Host bridge
    device pci 2.0 on end		# VGA (Intel 82830 CGC)
    chip southbridge/intel/i82801dx	# Southbridge
      register "pirqa_routing" = "0x05"
      register "pirqb_routing" = "0x06"
      register "pirqc_routing" = "0x07"
      register "pirqd_routing" = "0x09"
      register "pirqe_routing" = "0x0a"
      register "pirqf_routing" = "0x80"
      register "pirqg_routing" = "0x80"
      register "pirqh_routing" = "0x0b"

      register "ide0_enable" = "1"
      register "ide1_enable" = "1"

      device pci 1d.0 on end		# USB UHCI Controller #1
      device pci 1d.1 on end		# USB UHCI Controller #2
      device pci 1d.2 on end		# USB UHCI Controller #3
      device pci 1d.7 on end		# USB2 EHCI Controller
      device pci 1e.0 on end		# PCI bridge
      device pci 1f.0 on		# ISA/LPC bridge
        chip superio/smsc/smscsuperio	# Super I/O
          device pnp 2e.0 off		# Floppy
            io 0x60 = 0x3f0
            irq 0x70 = 6
            drq 0x74 = 2
          end
          device pnp 2e.3 on		# Parallel port
            io 0x60 = 0x378
            irq 0x70 = 7
            drq 0x74 = 4
          end
          device pnp 2e.4 on		# Com1
            io 0x60 = 0x3f8
            irq 0x70 = 4
          end
          device pnp 2e.5 on		# Com2 / IR
            io 0x60 = 0x2f8
            irq 0x70 = 3
          end
          device pnp 2e.7 on		# PS/2 keyboard/mouse
            io 0x60 = 0x60
            io 0x62 = 0x64
            irq 0x70 = 1		# Keyboard interrupt
            irq 0x72 = 12		# Mouse interrupt
          end
          device pnp 2e.9 off end	# Game port
          device pnp 2e.a on		# PME
            io 0x60 = 0x800
          end
          device pnp 2e.b off end	# MPU-401
        end
      end
      device pci 1f.1 on end		# IDE
      device pci 1f.3 on end		# SMBus
      device pci 1f.5 on end		# AC'97 audio
      device pci 1f.6 off end		# AC'97 modem
    end
  end
end

