chip northbridge/amd/amdk8/root_complex
        device lapic_cluster 0 on
                chip cpu/amd/socket_F
                        device lapic 0 on end
                end
        end

       device pci_domain 0 on
               chip northbridge/amd/amdk8 #mc0
                       device pci 18.0 on #  northbridge
                               #  devices on link 0, link 0 == LDT 0
                               chip southbridge/nvidia/mcp55
                                       device pci 0.0 on end   # HT
                                       device pci 1.0 on # LPC
                                               chip superio/winbond/w83627ehg
                                                       device pnp 2e.0 on #  Floppy
                                                               io 0x60 = 0x3f0
                                                               irq 0x70 = 6
                                                               drq 0x74 = 2
                                                       end
                                                       device pnp 2e.1 off #  Parallel Port
                                                               io 0x60 = 0x378
                                                               irq 0x70 = 7
                                                       end
                                                       device pnp 2e.2 on #  Com1
                                                               io 0x60 = 0x3f8
                                                               irq 0x70 = 4
                                                       end
                                                       device pnp 2e.3 off #  Com2
                                                               io 0x60 = 0x2f8
                                                               irq 0x70 = 3
                                                       end
                                                       device pnp 2e.5 on #  Keyboard
                                                               io 0x60 = 0x60
                                                               io 0x62 = 0x64
                                                               irq 0x70 = 1
                                                               irq 0x72 = 12
                                                       end
                                                       device pnp 2e.6 off #  SERIAL_FALSH
                                                               io 0x60 = 0x100
                                                       end
                                                       device pnp 2e.7 off #  GAME_MIDI_GIPO1
                                                               io 0x60 = 0x220
                                                               io 0x62 = 0x300
                                                               irq 0x70 = 9
                                                       end
                                                       device pnp 2e.8 off end #  WDTO_PLED
                                                       device pnp 2e.9 off end #  GPIO2_GPIO3_GPIO4_GPIO5
                                                       device pnp 2e.a off end #  ACPI
                                                       device pnp 2e.b on #  HW Monitor
                                                               io 0x60 = 0x290
                                                               irq 0x70 = 5
                                                       end
                                               end
                                       end
                                        device pci 1.1 on # SM 0
                                               chip drivers/i2c/i2cmux2 # pca9554 smbus mux
                                                       device i2c 70 on  #0 pca9554 1
                                                               chip drivers/generic/generic #dimm 0-0-0
                                                                        device i2c 50 on end
                                                                end
                                                                chip drivers/generic/generic #dimm 0-0-1
                                                                        device i2c 51 on end
                                                                end
                                                                chip drivers/generic/generic #dimm 0-1-0
                                                                        device i2c 52 on end
                                                                end
                                                                chip drivers/generic/generic #dimm 0-1-1
                                                                        device i2c 53 on end
                                                                end
                                                               chip drivers/generic/generic #dimm 0-0-0
                                                                        device i2c 54 on end
                                                                end
                                                                chip drivers/generic/generic #dimm 0-0-1
                                                                        device i2c 55 on end
                                                                end
                                                                chip drivers/generic/generic #dimm 0-1-0
                                                                        device i2c 56 on end
                                                                end
                                                                chip drivers/generic/generic #dimm 0-1-1
                                                                        device i2c 57 on end
                                                                end
                                                       end
                                                       device i2c 70 on  #0 pca9554 2
                                                               chip drivers/generic/generic #dimm 0-0-0
                                                                        device i2c 50 on end
                                                                end
                                                                chip drivers/generic/generic #dimm 0-0-1
                                                                        device i2c 51 on end
                                                                end
                                                                chip drivers/generic/generic #dimm 0-1-0
                                                                        device i2c 52 on end
                                                                end
                                                                chip drivers/generic/generic #dimm 0-1-1
                                                                        device i2c 53 on end
                                                                end
                                                               chip drivers/generic/generic #dimm 0-0-0
                                                                        device i2c 54 on end
                                                                end
                                                                chip drivers/generic/generic #dimm 0-0-1
                                                                        device i2c 55 on end
                                                                end
                                                                chip drivers/generic/generic #dimm 0-1-0
                                                                        device i2c 56 on end
                                                                end
                                                                chip drivers/generic/generic #dimm 0-1-1
                                                                        device i2c 57 on end
                                                                end
                                                       end
                                               end
                                       end
                                       device pci 1.1 on # SM 1
                                               chip drivers/i2c/i2cmux2 # pca9554 smbus mux
                                                       device i2c 72 on     #pca9554 channle1
                                                               chip drivers/i2c/adm1027   #HWM ADT7476 1
                                                                       device i2c 2e on end
                                                               end
                                                       end
                                                       device i2c 72 on     #pca9545 channel 2
                                                               chip drivers/i2c/adm1027   #HWM ADT7463
                                                                       device i2c 2e on end
                                                               end
                                                       end
                                                       device i2c 72 on end  #pca9545 channel 3
                                                       device i2c 72 on      #pca9545 channel 4
                                                               chip drivers/i2c/adm1027   #HWM ADT7476 2
                                                                       device i2c 2e on end
                                                               end
                                                       end
                                               end
                                       end

                                       device pci 2.0 on end # USB 1.1
                                       device pci 2.1 on end # USB 2
                                       device pci 4.0 on  end # IDE
                                               device pci 5.0 on  end # SATA 0
                                       device pci 5.1 on  end # SATA 1
                                       device pci 5.2 on  end # SATA 2
                                       device pci 6.0 on  #P2P
                                               device pci 4.0 on end
                                       end # P2P
                                       device pci 7.0 on end # reserve
                                       device pci 8.0 on end # MAC0
                                       device pci 9.0 on end # MAC1
                                       device pci a.0 on
                                               device pci 0.0 on
                                                       device pci 4.0 on end  #pci_E lan1
                                                       device pci 4.1 on end  #pci_E lan2
                                               end
                                       end # 0x376
                                               device pci b.0 on  end # PCI E 0x374
                                       device pci c.0 on  end
                                       device pci d.0 on   #SAS
                                               device pci 0.0 on end
                                       end # PCI E 1 0x378
                                       device pci e.0 on end # PCI E 0 0x375
                                       device pci f.0 on end   #PCI E 0x377  pci_E slot
                                       register "ide0_enable" = "1"
                                       register "ide1_enable" = "1"
                                       register "sata0_enable" = "1"
                                       register "sata1_enable" = "1"
                               end
                       end #  device pci 18.0
                       device pci 18.0 on end # Link 1
                       device pci 18.0 on end
                       device pci 18.1 on end
                       device pci 18.2 on end
                       device pci 18.3 on end
               end #mc0

       end # pci_domain

#        chip drivers/generic/debug
#                device pnp 0.0 off end
#                device pnp 0.1 off end
#                device pnp 0.2 off end
#                device pnp 0.3 off end
#                device pnp 0.4 off end
#              device pnp 0.5 on end
#        end
end # root_complex
