coreboot-4.0-r Tue May 31 22:39:21 CDT 2011 starting...
BSP Family_Model: 00500f10
cpu_init_detectedx = 00000000
Got past sb800_early_setup
BSP Family_Model: 00500f10
cpu_init_detectedx = 00000001
Got past sb800_early_setup
Got past agesawrapper_amdinitearly

EventLog:  EventClass = 2, EventInfo = 8040100.
  Param1 = a00a, Param2 = 0.
  Param3 = 0, Param4 = 0.

EventLog:  EventClass = 2, EventInfo = 8040100.
  Param1 = a00a, Param2 = 0.
  Param3 = 0, Param4 = 0.

EventLog:  EventClass = 2, EventInfo = 8040100.
  Param1 = a00a, Param2 = 0.
  Param3 = 0, Param4 = 0.

EventLog:  EventClass = 2, EventInfo = 8040100.
  Param1 = a00a, Param2 = 0.
  Param3 = 0, Param4 = 0.

EventLog:  EventClass = 2, EventInfo = 8040100.
  Param1 = a00a, Param2 = 0.
  Param3 = 0, Param4 = 0.

EventLog:  EventClass = 2, EventInfo = 8040100.
  Param1 = a00a, Param2 = 0.
  Param3 = 0, Param4 = 0.

EventLog:  EventClass = 2, EventInfo = 8040100.
  Param1 = a00a, Param2 = 0.
  Param3 = 0, Param4 = 0.

EventLog:  EventClass = 2, EventInfo = 8040100.
  Param1 = a00a, Param2 = 0.
  Param3 = 0, Param4 = 0.

EventLog:  EventClass = 2, EventInfo = 8040100.
  Param1 = a00a, Param2 = 0.
  Param3 = 0, Param4 = 0.

EventLog:  EventClass = 2, EventInfo = 8040100.
  Param1 = a00a, Param2 = 0.
  Param3 = 0, Param4 = 0.

EventLog:  EventClass = 2, EventInfo = 8040100.
  Param1 = a00a, Param2 = 0.
  Param3 = 0, Param4 = 0.

EventLog:  EventClass = 2, EventInfo = 8040100.
  Param1 = a00a, Param2 = 0.
  Param3 = 0, Param4 = 0.

EventLog:  EventClass = 2, EventInfo = 8040100.
  Param1 = a00a, Param2 = 0.
  Param3 = 0, Param4 = 0.

EventLog:  EventClass = 2, EventInfo = 8040100.
  Param1 = a00a, Param2 = 0.
  Param3 = 0, Param4 = 0.

EventLog:  EventClass = 2, EventInfo = 8040100.
  Param1 = a00a, Param2 = 0.
  Param3 = 0, Param4 = 0.

EventLog:  EventClass = 2, EventInfo = 8040100.
  Param1 = a00a, Param2 = 0.
  Param3 = 0, Param4 = 0.
agesawrapper_amdinitpost failed: 4
Got past agesawrapper_amdinitpost
Got past agesawrapper_amdinitenv
Loading image.
Check CBFS header at fffffcce
magic is 4f524243
Found CBFS header at fffffcce
Check cmos_layout.bin
CBFS: follow chain: ffc00000 + 28 + 6f0 + align -> ffc00740
Check pci1002,9802.rom
CBFS: follow chain: ffc00740 + 38 + e200 + align -> ffc0e980
Check fallback/romstage
CBFS: follow chain: ffc0e980 + 38 + 45fdc + align -> ffc549c0
Check fallback/coreboot_ram
Stage: loading fallback/coreboot_ram @ 0x200000 (1310720 bytes), entry @ 0x200000
Stage: done loading.
Jumping to image.
coreboot-4.0-r Tue May 31 22:39:21 CDT 2011 booting...
Enumerating buses...
Show all devs...Before device enumeration.
Root Device: enabled 1
APIC_CLUSTER: 0: enabled 1
APIC: 00: enabled 1
PCI_DOMAIN: 0000: enabled 1
PCI: 00:00.0: enabled 1
PCI: 00:01.0: enabled 1
PCI: 00:01.1: enabled 1
PCI: 00:04.0: enabled 1
PCI: 00:05.0: enabled 0
PCI: 00:06.0: enabled 0
PCI: 00:07.0: enabled 0
PCI: 00:08.0: enabled 0
PCI: 00:11.0: enabled 1
PCI: 00:12.0: enabled 1
PCI: 00:12.1: enabled 1
PCI: 00:12.2: enabled 1
PCI: 00:13.0: enabled 1
PCI: 00:13.1: enabled 1
PCI: 00:13.2: enabled 1
PCI: 00:14.0: enabled 1
I2C: 00:50: enabled 1
I2C: 00:51: enabled 1
PCI: 00:14.1: enabled 1
PCI: 00:14.2: enabled 1
PCI: 00:14.3: enabled 1
PNP: 004e.0: enabled 0
PNP: 004e.3: enabled 0
PNP: 004e.4: enabled 0
PNP: 004e.5: enabled 1
PNP: 004e.6: enabled 0
PNP: 004e.a: enabled 0
PNP: 004e.10: enabled 1
PNP: 004e.11: enabled 0
PCI: 00:14.4: enabled 1
PCI: 00:14.5: enabled 1
PCI: 00:15.0: enabled 0
PCI: 00:15.1: enabled 0
PCI: 00:15.2: enabled 0
PCI: 00:15.3: enabled 0
PCI: 00:18.0: enabled 1
PCI: 00:18.1: enabled 1
PCI: 00:18.2: enabled 1
PCI: 00:18.3: enabled 1
PCI: 00:18.4: enabled 1
PCI: 00:18.5: enabled 1
PCI: 00:18.6: enabled 1
PCI: 00:18.7: enabled 1
Compare with tree...
Root Device: enabled 1
 APIC_CLUSTER: 0: enabled 1
  APIC: 00: enabled 1
 PCI_DOMAIN: 0000: enabled 1
  PCI: 00:00.0: enabled 1
  PCI: 00:01.0: enabled 1
  PCI: 00:01.1: enabled 1
  PCI: 00:04.0: enabled 1
  PCI: 00:05.0: enabled 0
  PCI: 00:06.0: enabled 0
  PCI: 00:07.0: enabled 0
  PCI: 00:08.0: enabled 0
  PCI: 00:11.0: enabled 1
  PCI: 00:12.0: enabled 1
  PCI: 00:12.1: enabled 1
  PCI: 00:12.2: enabled 1
  PCI: 00:13.0: enabled 1
  PCI: 00:13.1: enabled 1
  PCI: 00:13.2: enabled 1
  PCI: 00:14.0: enabled 1
   I2C: 00:50: enabled 1
   I2C: 00:51: enabled 1
  PCI: 00:14.1: enabled 1
  PCI: 00:14.2: enabled 1
  PCI: 00:14.3: enabled 1
   PNP: 004e.0: enabled 0
   PNP: 004e.3: enabled 0
   PNP: 004e.4: enabled 0
   PNP: 004e.5: enabled 1
   PNP: 004e.6: enabled 0
   PNP: 004e.a: enabled 0
   PNP: 004e.10: enabled 1
   PNP: 004e.11: enabled 0
  PCI: 00:14.4: enabled 1
  PCI: 00:14.5: enabled 1
  PCI: 00:15.0: enabled 0
  PCI: 00:15.1: enabled 0
  PCI: 00:15.2: enabled 0
  PCI: 00:15.3: enabled 0
  PCI: 00:18.0: enabled 1
  PCI: 00:18.1: enabled 1
  PCI: 00:18.2: enabled 1
  PCI: 00:18.3: enabled 1
  PCI: 00:18.4: enabled 1
  PCI: 00:18.5: enabled 1
  PCI: 00:18.6: enabled 1
  PCI: 00:18.7: enabled 1
Mainboard Persimmon Enable.
persimmon_enable, TOP MEM: msr.lo = 0x7f000000, msr.hi = 0x00000000
persimmon_enable, TOP MEM2: msr2.lo = 0x00000000, msr2.hi = 0x00000000
persimmon_enable: uma size 0x18000000, memory start 0x67000000
scan_static_bus for Root Device
APIC_CLUSTER: 0 enabled
PCI_DOMAIN: 0000 enabled
PCI_DOMAIN: 0000 scanning...
PCI: pci_scan_bus for bus 00
PCI: Using configuration type 1
PCI: 00:00.0 [1022/1510] ops
PCI: 00:00.0 [1022/1510] enabled
PCI: 00:01.0 [1002/9802] enabled
PCI: 00:01.1 [1002/1314] enabled
Capability: type 0x01 @ 0x50
Capability: type 0x10 @ 0x58
Capability: type 0x05 @ 0xa0
Capability: type 0x0d @ 0xb0
Capability: type 0x08 @ 0xb8
Capability: type 0x01 @ 0x50
Capability: type 0x10 @ 0x58
PCI: 00:04.0 subordinate bus PCI Express
PCI: 00:04.0 [1022/1512] enabled
sb800_enable() PCI: 00:11.0 [1002/4391] ops
PCI: 00:11.0 [1002/4391] enabled
sb800_enable() PCI: 00:12.0 [1002/4397] ops
PCI: 00:12.0 [1002/4397] enabled
sb800_enable() PCI: Static device PCI: 00:12.1 not found, disabling it.
sb800_enable() PCI: 00:12.2 [1002/4396] ops
PCI: 00:12.2 [1002/4396] enabled
sb800_enable() PCI: 00:13.0 [1002/4397] ops
PCI: 00:13.0 [1002/4397] enabled
sb800_enable() PCI: Static device PCI: 00:13.1 not found, disabling it.
sb800_enable() PCI: 00:13.2 [1002/4396] ops
PCI: 00:13.2 [1002/4396] enabled
sb800_enable() sm_init().
IOAPIC: Clearing IOAPIC at 0xfec00000
IOAPIC: 23 interrupts
IOAPIC: reg 0x00000000 value 0x00000000 0x00010000
IOAPIC: reg 0x00000001 value 0x00000000 0x00010000
IOAPIC: reg 0x00000002 value 0x00000000 0x00010000
IOAPIC: reg 0x00000003 value 0x00000000 0x00010000
IOAPIC: reg 0x00000004 value 0x00000000 0x00010000
IOAPIC: reg 0x00000005 value 0x00000000 0x00010000
IOAPIC: reg 0x00000006 value 0x00000000 0x00010000
IOAPIC: reg 0x00000007 value 0x00000000 0x00010000
IOAPIC: reg 0x00000008 value 0x00000000 0x00010000
IOAPIC: reg 0x00000009 value 0x00000000 0x00010000
IOAPIC: reg 0x0000000a value 0x00000000 0x00010000
IOAPIC: reg 0x0000000b value 0x00000000 0x00010000
IOAPIC: reg 0x0000000c value 0x00000000 0x00010000
IOAPIC: reg 0x0000000d value 0x00000000 0x00010000
IOAPIC: reg 0x0000000e value 0x00000000 0x00010000
IOAPIC: reg 0x0000000f value 0x00000000 0x00010000
IOAPIC: reg 0x00000010 value 0x00000000 0x00010000
IOAPIC: reg 0x00000011 value 0x00000000 0x00010000
IOAPIC: reg 0x00000012 value 0x00000000 0x00010000
IOAPIC: reg 0x00000013 value 0x00000000 0x00010000
IOAPIC: reg 0x00000014 value 0x00000000 0x00010000
IOAPIC: reg 0x00000015 value 0x00000000 0x00010000
IOAPIC: reg 0x00000016 value 0x00000000 0x00010000
IOAPIC: Initializing IOAPIC at 0xfec00000
IOAPIC: Bootstrap Processor Local APIC = 0x00
IOAPIC: ID = 0x02
IOAPIC: 23 interrupts
IOAPIC: Enabling interrupts on FSB
IOAPIC: reg 0x00000000 value 0x00000000 0x00000700
IOAPIC: reg 0x00000001 value 0x00000000 0x00010000
IOAPIC: reg 0x00000002 value 0x00000000 0x00010000
IOAPIC: reg 0x00000003 value 0x00000000 0x00010000
IOAPIC: reg 0x00000004 value 0x00000000 0x00010000
IOAPIC: reg 0x00000005 value 0x00000000 0x00010000
IOAPIC: reg 0x00000006 value 0x00000000 0x00010000
IOAPIC: reg 0x00000007 value 0x00000000 0x00010000
IOAPIC: reg 0x00000008 value 0x00000000 0x00010000
IOAPIC: reg 0x00000009 value 0x00000000 0x00010000
IOAPIC: reg 0x0000000a value 0x00000000 0x00010000
IOAPIC: reg 0x0000000b value 0x00000000 0x00010000
IOAPIC: reg 0x0000000c value 0x00000000 0x00010000
IOAPIC: reg 0x0000000d value 0x00000000 0x00010000
IOAPIC: reg 0x0000000e value 0x00000000 0x00010000
IOAPIC: reg 0x0000000f value 0x00000000 0x00010000
IOAPIC: reg 0x00000010 value 0x00000000 0x00010000
IOAPIC: reg 0x00000011 value 0x00000000 0x00010000
IOAPIC: reg 0x00000012 value 0x00000000 0x00010000
IOAPIC: reg 0x00000013 value 0x00000000 0x00010000
IOAPIC: reg 0x00000014 value 0x00000000 0x00010000
IOAPIC: reg 0x00000015 value 0x00000000 0x00010000
IOAPIC: reg 0x00000016 value 0x00000000 0x00010000
PCI: 00:14.0 [1002/4385] enabled
sb800_enable() PCI: Static device PCI: 00:14.1 not found, disabling it.
sb800_enable() hda enabled
PCI: 00:14.2 [1002/4383] ops
PCI: 00:14.2 [1002/4383] enabled
sb800_enable() PCI: 00:14.3 [1002/439d] bus ops
PCI: 00:14.3 [1002/439d] enabled
sb800_enable() PCI: 00:14.4 [1002/4384] bus ops
PCI: 00:14.4 [1002/4384] enabled
sb800_enable() PCI: 00:14.5 [1002/4399] ops
PCI: 00:14.5 [1002/4399] enabled
sb800_enable() sb800_enable() sb800_enable() sb800_enable() PCI: 00:16.0 [1002/4397] ops
PCI: 00:16.0 [1002/4397] enabled
PCI: 00:16.2 [1002/4396] ops
PCI: 00:16.2 [1002/4396] enabled
PCI: 00:18.0 [1022/1700] enabled
PCI: 00:18.1 [1022/1701] enabled
PCI: 00:18.2 [1022/1702] enabled
PCI: 00:18.3 [1022/1703] enabled
PCI: 00:18.4 [1022/1704] enabled
PCI: 00:18.5 [1022/1718] enabled
PCI: 00:18.6 [1022/1716] enabled
PCI: 00:18.7 [1022/1719] enabled
do_pci_scan_bridge for PCI: 00:04.0
PCI: pci_scan_bus for bus 01
PCI: 01:00.0 [10ec/8168] enabled
PCI: pci_scan_bus returning with max=001
Capability: type 0x01 @ 0x40
Capability: type 0x05 @ 0x50
Capability: type 0x10 @ 0x70
do_pci_scan_bridge returns max 1
scan_static_bus for PCI: 00:14.3
PNP: 004e.0 disabled
PNP: 004e.3 disabled
PNP: 004e.4 disabled
PNP: 004e.5 enabled
PNP: 004e.6 disabled
PNP: 004e.a disabled
PNP: 004e.10 enabled
PNP: 004e.11 disabled
scan_static_bus for PCI: 00:14.3 done
do_pci_scan_bridge for PCI: 00:14.4
PCI: pci_scan_bus for bus 02
PCI: pci_scan_bus returning with max=002
do_pci_scan_bridge returns max 2
PCI: pci_scan_bus returning with max=002
scan_static_bus for Root Device done
done
Setting up VGA for PCI: 00:01.0
Setting PCI_BRIDGE_CTL_VGA for bridge PCI_DOMAIN: 0000
Setting PCI_BRIDGE_CTL_VGA for bridge Root Device
Allocating resources...
Reading resources...
Root Device read_resources bus 0 link: 0

Fam14h - cpu_bus_read_resources.
APIC_CLUSTER: 0 read_resources bus 0 link: 0
APIC: 00 missing read_resources
APIC_CLUSTER: 0 read_resources bus 0 link: 0 done

Fam14h - domain_read_resources.
PCI_DOMAIN: 0000 read_resources bus 0 link: 0

Fam14h - read_resources.
PCI: 00:04.0 read_resources bus 1 link: 0
PCI: 00:04.0 read_resources bus 1 link: 0 done
PCI: 00:14.0 read_resources bus 0 link: 0
I2C: 00:50 missing read_resources
I2C: 00:51 missing read_resources
PCI: 00:14.0 read_resources bus 0 link: 0 done
PCI: 00:14.3 read_resources bus 0 link: 0
PCI: 00:14.3 read_resources bus 0 link: 0 done
PCI: 00:14.4 read_resources bus 2 link: 0
PCI: 00:14.4 read_resources bus 2 link: 0 done
PCI_DOMAIN: 0000 read_resources bus 0 link: 0 done
Root Device read_resources bus 0 link: 0 done
Done reading resources.
Show resources in subtree (Root Device)...After reading.
 Root Device child on link 0 APIC_CLUSTER: 0
  APIC_CLUSTER: 0 child on link 0 APIC: 00
  APIC_CLUSTER: 0 resource base f8000000 size 1000000 align 0 gran 0 limit 0 flags f0000200 index c0010058
   APIC: 00
  PCI_DOMAIN: 0000 child on link 0 PCI: 00:00.0
  PCI_DOMAIN: 0000 resource base 0 size 0 align 0 gran 0 limit ffff flags 40040100 index 10000000
  PCI_DOMAIN: 0000 resource base 0 size 0 align 0 gran 0 limit ffffffff flags 40040200 index 10000100
   PCI: 00:00.0
   PCI: 00:01.0
   PCI: 00:01.0 resource base 0 size 10000000 align 28 gran 28 limit ffffffff flags 1200 index 10
   PCI: 00:01.0 resource base 0 size 100 align 8 gran 8 limit ffff flags 100 index 14
   PCI: 00:01.0 resource base 0 size 40000 align 18 gran 18 limit ffffffff flags 200 index 18
   PCI: 00:01.1
   PCI: 00:01.1 resource base 0 size 4000 align 14 gran 14 limit ffffffff flags 200 index 10
   PCI: 00:04.0 child on link 0 PCI: 01:00.0
   PCI: 00:04.0 resource base 0 size 0 align 12 gran 12 limit ffffffff flags 80102 index 1c
   PCI: 00:04.0 resource base 0 size 0 align 20 gran 20 limit ffffffffffffffff flags 81202 index 24
   PCI: 00:04.0 resource base 0 size 0 align 20 gran 20 limit ffffffff flags 80202 index 20
    PCI: 01:00.0
    PCI: 01:00.0 resource base 0 size 100 align 8 gran 8 limit ffff flags 100 index 10
    PCI: 01:00.0 resource base 0 size 1000 align 12 gran 12 limit ffffffffffffffff flags 1201 index 18
    PCI: 01:00.0 resource base 0 size 4000 align 14 gran 14 limit ffffffffffffffff flags 1201 index 20
    PCI: 01:00.0 resource base 0 size 20000 align 17 gran 17 limit ffffffff flags 2200 index 30
   PCI: 00:05.0
   PCI: 00:06.0
   PCI: 00:07.0
   PCI: 00:08.0
   PCI: 00:11.0
   PCI: 00:11.0 resource base 0 size 8 align 3 gran 3 limit ffff flags 100 index 10
   PCI: 00:11.0 resource base 0 size 4 align 2 gran 2 limit ffff flags 100 index 14
   PCI: 00:11.0 resource base 0 size 8 align 3 gran 3 limit ffff flags 100 index 18
   PCI: 00:11.0 resource base 0 size 4 align 2 gran 2 limit ffff flags 100 index 1c
   PCI: 00:11.0 resource base 0 size 10 align 4 gran 4 limit ffff flags 100 index 20
   PCI: 00:11.0 resource base 0 size 400 align 10 gran 10 limit ffffffff flags 200 index 24
   PCI: 00:12.0
   PCI: 00:12.0 resource base 0 size 1000 align 12 gran 12 limit ffffffff flags 200 index 10
   PCI: 00:12.1
   PCI: 00:12.2
   PCI: 00:12.2 resource base 0 size 100 align 8 gran 8 limit ffffffff flags 200 index 10
   PCI: 00:13.0
   PCI: 00:13.0 resource base 0 size 1000 align 12 gran 12 limit ffffffff flags 200 index 10
   PCI: 00:13.1
   PCI: 00:13.2
   PCI: 00:13.2 resource base 0 size 100 align 8 gran 8 limit ffffffff flags 200 index 10
   PCI: 00:14.0 child on link 0 I2C: 00:50
    I2C: 00:50
    I2C: 00:51
   PCI: 00:14.1
   PCI: 00:14.2
   PCI: 00:14.2 resource base 0 size 4000 align 14 gran 14 limit ffffffffffffffff flags 201 index 10
   PCI: 00:14.3 child on link 0 PNP: 004e.0
   PCI: 00:14.3 resource base 0 size 1 align 0 gran 0 limit ffffffff flags 200 index a0
   PCI: 00:14.3 resource base 0 size 1000 align 0 gran 0 limit 0 flags c0040100 index 10000000
   PCI: 00:14.3 resource base ff800000 size 800000 align 0 gran 0 limit 0 flags c0040200 index 10000100
   PCI: 00:14.3 resource base fec00000 size 1000 align 0 gran 0 limit 0 flags c0000200 index 3
    PNP: 004e.0
    PNP: 004e.0 resource base 3f0 size 8 align 3 gran 3 limit 7ff flags c0000100 index 60
    PNP: 004e.0 resource base 6 size 1 align 0 gran 0 limit 0 flags c0000400 index 70
    PNP: 004e.0 resource base 2 size 1 align 0 gran 0 limit 0 flags c0000800 index 74
    PNP: 004e.3
    PNP: 004e.3 resource base 0 size 8 align 3 gran 3 limit 7ff flags 100 index 60
    PNP: 004e.3 resource base 0 size 1 align 0 gran 0 limit 0 flags 400 index 70
    PNP: 004e.3 resource base 0 size 1 align 0 gran 0 limit 0 flags 800 index 74
    PNP: 004e.4
    PNP: 004e.4 resource base 0 size 8 align 3 gran 3 limit fff flags 100 index 60
    PNP: 004e.4 resource base 0 size 1 align 0 gran 0 limit 0 flags 400 index 70
    PNP: 004e.5
    PNP: 004e.5 resource base 60 size 1 align 0 gran 0 limit ffffffff flags c0000100 index 60
    PNP: 004e.5 resource base 64 size 0 align 0 gran 0 limit 0 flags c0000100 index 62
    PNP: 004e.5 resource base 1 size 1 align 0 gran 0 limit 0 flags c0000400 index 70
    PNP: 004e.5 resource base 0 size 1 align 0 gran 0 limit 0 flags 400 index 72
    PNP: 004e.6
    PNP: 004e.6 resource base 0 size 1 align 0 gran 0 limit 0 flags 400 index 70
    PNP: 004e.a
    PNP: 004e.10
    PNP: 004e.10 resource base 3f8 size 8 align 3 gran 3 limit 7ff flags c0000100 index 60
    PNP: 004e.10 resource base 4 size 1 align 0 gran 0 limit 0 flags c0000400 index 70
    PNP: 004e.11
    PNP: 004e.11 resource base 2f8 size 8 align 3 gran 3 limit 7ff flags c0000100 index 60
    PNP: 004e.11 resource base 3 size 1 align 0 gran 0 limit 0 flags c0000400 index 70
   PCI: 00:14.4
   PCI: 00:14.4 resource base 0 size 0 align 12 gran 12 limit ffff flags 80102 index 1c
   PCI: 00:14.4 resource base 0 size 0 align 20 gran 20 limit ffffffff flags 81202 index 24
   PCI: 00:14.4 resource base 0 size 0 align 20 gran 20 limit ffffffff flags 80202 index 20
   PCI: 00:14.5
   PCI: 00:14.5 resource base 0 size 1000 align 12 gran 12 limit ffffffff flags 200 index 10
   PCI: 00:15.0
   PCI: 00:15.1
   PCI: 00:15.2
   PCI: 00:15.3
   PCI: 00:16.0
   PCI: 00:16.0 resource base 0 size 1000 align 12 gran 12 limit ffffffff flags 200 index 10
   PCI: 00:16.2
   PCI: 00:16.2 resource base 0 size 100 align 8 gran 8 limit ffffffff flags 200 index 10
   PCI: 00:18.0
   PCI: 00:18.1
   PCI: 00:18.2
   PCI: 00:18.3
   PCI: 00:18.4
   PCI: 00:18.5
   PCI: 00:18.6
   PCI: 00:18.7
PCI_DOMAIN: 0000 compute_resources_io: base: 0 size: 0 align: 0 gran: 0 limit: ffff
PCI: 00:04.0 compute_resources_io: base: 0 size: 0 align: 12 gran: 12 limit: ffffffff
PCI: 01:00.0 10 *  [0x0 - 0xff] io
PCI: 00:04.0 compute_resources_io: base: 100 size: 1000 align: 12 gran: 12 limit: ffff done
PCI: 00:14.4 compute_resources_io: base: 0 size: 0 align: 12 gran: 12 limit: ffff
PCI: 00:14.4 compute_resources_io: base: 0 size: 0 align: 12 gran: 12 limit: ffff done
PCI: 00:04.0 1c *  [0x0 - 0xfff] io
PCI: 00:01.0 14 *  [0x1000 - 0x10ff] io
PCI: 00:11.0 20 *  [0x1400 - 0x140f] io
PCI: 00:11.0 10 *  [0x1410 - 0x1417] io
PCI: 00:11.0 18 *  [0x1418 - 0x141f] io
PCI: 00:11.0 14 *  [0x1420 - 0x1423] io
PCI: 00:11.0 1c *  [0x1424 - 0x1427] io
PCI_DOMAIN: 0000 compute_resources_io: base: 1428 size: 1428 align: 12 gran: 0 limit: ffff done
PCI_DOMAIN: 0000 compute_resources_mem: base: 0 size: 0 align: 0 gran: 0 limit: ffffffff
PCI: 00:04.0 compute_resources_prefmem: base: 0 size: 0 align: 20 gran: 20 limit: ffffffffffffffff
PCI: 01:00.0 20 *  [0x0 - 0x3fff] prefmem
PCI: 01:00.0 18 *  [0x4000 - 0x4fff] prefmem
PCI: 00:04.0 compute_resources_prefmem: base: 5000 size: 100000 align: 20 gran: 20 limit: ffffffffffffffff done
PCI: 00:04.0 compute_resources_mem: base: 0 size: 0 align: 20 gran: 20 limit: ffffffff
PCI: 01:00.0 30 *  [0x0 - 0x1ffff] mem
PCI: 00:04.0 compute_resources_mem: base: 20000 size: 100000 align: 20 gran: 20 limit: ffffffff done
PCI: 00:14.4 compute_resources_prefmem: base: 0 size: 0 align: 20 gran: 20 limit: ffffffff
PCI: 00:14.4 compute_resources_prefmem: base: 0 size: 0 align: 20 gran: 20 limit: ffffffff done
PCI: 00:14.4 compute_resources_mem: base: 0 size: 0 align: 20 gran: 20 limit: ffffffff
PCI: 00:14.4 compute_resources_mem: base: 0 size: 0 align: 20 gran: 20 limit: ffffffff done
PCI: 00:01.0 10 *  [0x0 - 0xfffffff] prefmem
PCI: 00:04.0 24 *  [0x10000000 - 0x100fffff] prefmem
PCI: 00:04.0 20 *  [0x10100000 - 0x101fffff] mem
PCI: 00:01.0 18 *  [0x10200000 - 0x1023ffff] mem
PCI: 00:01.1 10 *  [0x10240000 - 0x10243fff] mem
PCI: 00:14.2 10 *  [0x10244000 - 0x10247fff] mem
PCI: 00:12.0 10 *  [0x10248000 - 0x10248fff] mem
PCI: 00:13.0 10 *  [0x10249000 - 0x10249fff] mem
PCI: 00:14.5 10 *  [0x1024a000 - 0x1024afff] mem
PCI: 00:16.0 10 *  [0x1024b000 - 0x1024bfff] mem
PCI: 00:11.0 24 *  [0x1024c000 - 0x1024c3ff] mem
PCI: 00:12.2 10 *  [0x1024c400 - 0x1024c4ff] mem
PCI: 00:13.2 10 *  [0x1024c500 - 0x1024c5ff] mem
PCI: 00:16.2 10 *  [0x1024c600 - 0x1024c6ff] mem
PCI: 00:14.3 a0 *  [0x1024c700 - 0x1024c700] mem
PCI_DOMAIN: 0000 compute_resources_mem: base: 1024c701 size: 1024c701 align: 28 gran: 0 limit: ffffffff done
avoid_fixed_resources: PCI_DOMAIN: 0000
avoid_fixed_resources:@PCI_DOMAIN: 0000 10000000 limit 0000ffff
avoid_fixed_resources:@PCI_DOMAIN: 0000 10000100 limit ffffffff
constrain_resources: PCI_DOMAIN: 0000
constrain_resources: PCI: 00:00.0
constrain_resources: PCI: 00:01.0
constrain_resources: PCI: 00:01.1
constrain_resources: PCI: 00:04.0
constrain_resources: PCI: 01:00.0
constrain_resources: PCI: 00:11.0
constrain_resources: PCI: 00:12.0
constrain_resources: PCI: 00:12.2
constrain_resources: PCI: 00:13.0
constrain_resources: PCI: 00:13.2
constrain_resources: PCI: 00:14.0
constrain_resources: I2C: 00:50
constrain_resources: I2C: 00:51
constrain_resources: PCI: 00:14.2
constrain_resources: PCI: 00:14.3
constrain_resources: PNP: 004e.5
skipping PNP: 004e.5@62 fixed resource, size=0!
constrain_resources: PNP: 004e.10
constrain_resources: PCI: 00:14.4
constrain_resources: PCI: 00:14.5
constrain_resources: PCI: 00:16.0
constrain_resources: PCI: 00:16.2
constrain_resources: PCI: 00:18.0
constrain_resources: PCI: 00:18.1
constrain_resources: PCI: 00:18.2
constrain_resources: PCI: 00:18.3
constrain_resources: PCI: 00:18.4
constrain_resources: PCI: 00:18.5
constrain_resources: PCI: 00:18.6
constrain_resources: PCI: 00:18.7
avoid_fixed_resources2: PCI_DOMAIN: 0000@10000000 limit 0000ffff
        lim->base 00001000 lim->limit 0000ffff
avoid_fixed_resources2: PCI_DOMAIN: 0000@10000100 limit ffffffff
        lim->base 00000000 lim->limit febfffff
Setting resources...
PCI_DOMAIN: 0000 allocate_resources_io: base:1000 size:1428 align:12 gran:0 limit:ffff
Assigned: PCI: 00:04.0 1c *  [0x1000 - 0x1fff] io
Assigned: PCI: 00:01.0 14 *  [0x2000 - 0x20ff] io
Assigned: PCI: 00:11.0 20 *  [0x2400 - 0x240f] io
Assigned: PCI: 00:11.0 10 *  [0x2410 - 0x2417] io
Assigned: PCI: 00:11.0 18 *  [0x2418 - 0x241f] io
Assigned: PCI: 00:11.0 14 *  [0x2420 - 0x2423] io
Assigned: PCI: 00:11.0 1c *  [0x2424 - 0x2427] io
PCI_DOMAIN: 0000 allocate_resources_io: next_base: 2428 size: 1428 align: 12 gran: 0 done
PCI: 00:04.0 allocate_resources_io: base:1000 size:1000 align:12 gran:12 limit:ffff
Assigned: PCI: 01:00.0 10 *  [0x1000 - 0x10ff] io
PCI: 00:04.0 allocate_resources_io: next_base: 1100 size: 1000 align: 12 gran: 12 done
PCI: 00:14.4 allocate_resources_io: base:ffff size:0 align:12 gran:12 limit:ffff
PCI: 00:14.4 allocate_resources_io: next_base: ffff size: 0 align: 12 gran: 12 done
PCI_DOMAIN: 0000 allocate_resources_mem: base:e0000000 size:1024c701 align:28 gran:0 limit:febfffff
Assigned: PCI: 00:01.0 10 *  [0xe0000000 - 0xefffffff] prefmem
Assigned: PCI: 00:04.0 24 *  [0xf0000000 - 0xf00fffff] prefmem
Assigned: PCI: 00:04.0 20 *  [0xf0100000 - 0xf01fffff] mem
Assigned: PCI: 00:01.0 18 *  [0xf0200000 - 0xf023ffff] mem
Assigned: PCI: 00:01.1 10 *  [0xf0240000 - 0xf0243fff] mem
Assigned: PCI: 00:14.2 10 *  [0xf0244000 - 0xf0247fff] mem
Assigned: PCI: 00:12.0 10 *  [0xf0248000 - 0xf0248fff] mem
Assigned: PCI: 00:13.0 10 *  [0xf0249000 - 0xf0249fff] mem
Assigned: PCI: 00:14.5 10 *  [0xf024a000 - 0xf024afff] mem
Assigned: PCI: 00:16.0 10 *  [0xf024b000 - 0xf024bfff] mem
Assigned: PCI: 00:11.0 24 *  [0xf024c000 - 0xf024c3ff] mem
Assigned: PCI: 00:12.2 10 *  [0xf024c400 - 0xf024c4ff] mem
Assigned: PCI: 00:13.2 10 *  [0xf024c500 - 0xf024c5ff] mem
Assigned: PCI: 00:16.2 10 *  [0xf024c600 - 0xf024c6ff] mem
Assigned: PCI: 00:14.3 a0 *  [0xf024c700 - 0xf024c700] mem
PCI_DOMAIN: 0000 allocate_resources_mem: next_base: f024c701 size: 1024c701 align: 28 gran: 0 done
PCI: 00:04.0 allocate_resources_prefmem: base:f0000000 size:100000 align:20 gran:20 limit:febfffff
Assigned: PCI: 01:00.0 20 *  [0xf0000000 - 0xf0003fff] prefmem
Assigned: PCI: 01:00.0 18 *  [0xf0004000 - 0xf0004fff] prefmem
PCI: 00:04.0 allocate_resources_prefmem: next_base: f0005000 size: 100000 align: 20 gran: 20 done
PCI: 00:04.0 allocate_resources_mem: base:f0100000 size:100000 align:20 gran:20 limit:febfffff
Assigned: PCI: 01:00.0 30 *  [0xf0100000 - 0xf011ffff] mem
PCI: 00:04.0 allocate_resources_mem: next_base: f0120000 size: 100000 align: 20 gran: 20 done
PCI: 00:14.4 allocate_resources_prefmem: base:febfffff size:0 align:20 gran:20 limit:febfffff
PCI: 00:14.4 allocate_resources_prefmem: next_base: febfffff size: 0 align: 20 gran: 20 done
PCI: 00:14.4 allocate_resources_mem: base:febfffff size:0 align:20 gran:20 limit:febfffff
PCI: 00:14.4 allocate_resources_mem: next_base: febfffff size: 0 align: 20 gran: 20 done
Root Device assign_resources, bus 0 link: 0

Fam14h - cpu_bus_set_resources.
APIC_CLUSTER: 0 c0010058 <- [0x00f8000000 - 0x00f8ffffff] size 0x01000000 gran 0x00 mem <mmconfig>
APIC_CLUSTER: 0 assign_resources, bus 0 link: 0
APIC_CLUSTER: 0 assign_resources, bus 0 link: 0

Fam14h - domain_set_resources.
  amsr - incoming dev = 0024b3a0
adsr: (before) basek = 0, limitk = 7effffff.
adsr: (after) basek = 0, limitk = 1fbfff, sizek = 1fc000.
adsr - 0xa0000 to 0xbffff resource.
adsr: mmio_basek=00380000, basek=00000300, limitk=00000000
0: mmio_basek=00380000, basek=00000300, limitk=001fbfff
  adsr - uma_memory_base = 67000000.
  adsr - mmio_basek = 380000.
  adsr - high_tables_size = 10000.
adsr - adding uma resource.

Fam14h - Adding UMA memory.
PCI_DOMAIN: 0000 assign_resources, bus 0 link: 0
PCI: 00:01.0 10 <- [0x00e0000000 - 0x00efffffff] size 0x10000000 gran 0x1c prefmem
PCI: 00:01.0 14 <- [0x0000002000 - 0x00000020ff] size 0x00000100 gran 0x08 io
PCI: 00:01.0 18 <- [0x00f0200000 - 0x00f023ffff] size 0x00040000 gran 0x12 mem
PCI: 00:01.1 10 <- [0x00f0240000 - 0x00f0243fff] size 0x00004000 gran 0x0e mem
PCI: 00:04.0 1c <- [0x0000001000 - 0x0000001fff] size 0x00001000 gran 0x0c bus 01 io
PCI: 00:04.0 24 <- [0x00f0000000 - 0x00f00fffff] size 0x00100000 gran 0x14 bus 01 prefmem
PCI: 00:04.0 20 <- [0x00f0100000 - 0x00f01fffff] size 0x00100000 gran 0x14 bus 01 mem
PCI: 00:04.0 assign_resources, bus 1 link: 0
PCI: 01:00.0 10 <- [0x0000001000 - 0x00000010ff] size 0x00000100 gran 0x08 io
PCI: 01:00.0 18 <- [0x00f0004000 - 0x00f0004fff] size 0x00001000 gran 0x0c prefmem64
PCI: 01:00.0 20 <- [0x00f0000000 - 0x00f0003fff] size 0x00004000 gran 0x0e prefmem64
PCI: 01:00.0 30 <- [0x00f0100000 - 0x00f011ffff] size 0x00020000 gran 0x11 romem
PCI: 00:04.0 assign_resources, bus 1 link: 0
PCI: 00:11.0 10 <- [0x0000002410 - 0x0000002417] size 0x00000008 gran 0x03 io
PCI: 00:11.0 14 <- [0x0000002420 - 0x0000002423] size 0x00000004 gran 0x02 io
PCI: 00:11.0 18 <- [0x0000002418 - 0x000000241f] size 0x00000008 gran 0x03 io
PCI: 00:11.0 1c <- [0x0000002424 - 0x0000002427] size 0x00000004 gran 0x02 io
PCI: 00:11.0 20 <- [0x0000002400 - 0x000000240f] size 0x00000010 gran 0x04 io
PCI: 00:11.0 24 <- [0x00f024c000 - 0x00f024c3ff] size 0x00000400 gran 0x0a mem
PCI: 00:12.0 10 <- [0x00f0248000 - 0x00f0248fff] size 0x00001000 gran 0x0c mem
PCI: 00:12.2 10 <- [0x00f024c400 - 0x00f024c4ff] size 0x00000100 gran 0x08 mem
PCI: 00:13.0 10 <- [0x00f0249000 - 0x00f0249fff] size 0x00001000 gran 0x0c mem
PCI: 00:13.2 10 <- [0x00f024c500 - 0x00f024c5ff] size 0x00000100 gran 0x08 mem
PCI: 00:14.2 10 <- [0x00f0244000 - 0x00f0247fff] size 0x00004000 gran 0x0e mem64
PCI: 00:14.3 a0 <- [0x00f024c700 - 0x00f024c700] size 0x00000001 gran 0x00 mem
PCI: 00:14.3 assign_resources, bus 0 link: 0
PNP: 004e.5 60 <- [0x0000000060 - 0x0000000060] size 0x00000001 gran 0x00 io
PNP: 004e.5 62 <- [0x0000000064 - 0x0000000063] size 0x00000000 gran 0x00 io
PNP: 004e.5 70 <- [0x0000000001 - 0x0000000001] size 0x00000001 gran 0x00 irq
ERROR: PNP: 004e.5 72 irq size: 0x0000000001 not assigned
PNP: 004e.10 60 <- [0x00000003f8 - 0x00000003ff] size 0x00000008 gran 0x03 io
PNP: 004e.10 70 <- [0x0000000004 - 0x0000000004] size 0x00000001 gran 0x00 irq
PCI: 00:14.3 assign_resources, bus 0 link: 0
PCI: 00:14.4 1c <- [0x000000ffff - 0x000000fffe] size 0x00000000 gran 0x0c bus 02 io
PCI: 00:14.4 24 <- [0x00febfffff - 0x00febffffe] size 0x00000000 gran 0x14 bus 02 prefmem
PCI: 00:14.4 20 <- [0x00febfffff - 0x00febffffe] size 0x00000000 gran 0x14 bus 02 mem
PCI: 00:14.5 10 <- [0x00f024a000 - 0x00f024afff] size 0x00001000 gran 0x0c mem
PCI: 00:16.0 10 <- [0x00f024b000 - 0x00f024bfff] size 0x00001000 gran 0x0c mem
PCI: 00:16.2 10 <- [0x00f024c600 - 0x00f024c6ff] size 0x00000100 gran 0x08 mem
PCI_DOMAIN: 0000 assign_resources, bus 0 link: 0
  adsr - leaving this lovely routine.
Root Device assign_resources, bus 0 link: 0
Done setting resources.
Show resources in subtree (Root Device)...After assigning values.
 Root Device child on link 0 APIC_CLUSTER: 0
  APIC_CLUSTER: 0 child on link 0 APIC: 00
  APIC_CLUSTER: 0 resource base f8000000 size 1000000 align 0 gran 0 limit 0 flags f0000200 index c0010058
   APIC: 00
  PCI_DOMAIN: 0000 child on link 0 PCI: 00:00.0
  PCI_DOMAIN: 0000 resource base 1000 size 1428 align 12 gran 0 limit ffff flags 40040100 index 10000000
  PCI_DOMAIN: 0000 resource base e0000000 size 1024c701 align 28 gran 0 limit febfffff flags 40040200 index 10000100
  PCI_DOMAIN: 0000 resource base 0 size a0000 align 0 gran 0 limit 0 flags e0004200 index 10
  PCI_DOMAIN: 0000 resource base c0000 size 7ef3fc00 align 0 gran 0 limit 0 flags e0004200 index 20
  PCI_DOMAIN: 0000 resource base 67000000 size 18000000 align 0 gran 0 limit 0 flags f0000200 index 7
   PCI: 00:00.0
   PCI: 00:01.0
   PCI: 00:01.0 resource base e0000000 size 10000000 align 28 gran 28 limit febfffff flags 60001200 index 10
   PCI: 00:01.0 resource base 2000 size 100 align 8 gran 8 limit ffff flags 60000100 index 14
   PCI: 00:01.0 resource base f0200000 size 40000 align 18 gran 18 limit febfffff flags 60000200 index 18
   PCI: 00:01.1
   PCI: 00:01.1 resource base f0240000 size 4000 align 14 gran 14 limit febfffff flags 60000200 index 10
   PCI: 00:04.0 child on link 0 PCI: 01:00.0
   PCI: 00:04.0 resource base 1000 size 1000 align 12 gran 12 limit ffff flags 60080102 index 1c
   PCI: 00:04.0 resource base f0000000 size 100000 align 20 gran 20 limit febfffff flags 60081202 index 24
   PCI: 00:04.0 resource base f0100000 size 100000 align 20 gran 20 limit febfffff flags 60080202 index 20
    PCI: 01:00.0
    PCI: 01:00.0 resource base 1000 size 100 align 8 gran 8 limit ffff flags 60000100 index 10
    PCI: 01:00.0 resource base f0004000 size 1000 align 12 gran 12 limit febfffff flags 60001201 index 18
    PCI: 01:00.0 resource base f0000000 size 4000 align 14 gran 14 limit febfffff flags 60001201 index 20
    PCI: 01:00.0 resource base f0100000 size 20000 align 17 gran 17 limit febfffff flags 60002200 index 30
   PCI: 00:05.0
   PCI: 00:06.0
   PCI: 00:07.0
   PCI: 00:08.0
   PCI: 00:11.0
   PCI: 00:11.0 resource base 2410 size 8 align 3 gran 3 limit ffff flags 60000100 index 10
   PCI: 00:11.0 resource base 2420 size 4 align 2 gran 2 limit ffff flags 60000100 index 14
   PCI: 00:11.0 resource base 2418 size 8 align 3 gran 3 limit ffff flags 60000100 index 18
   PCI: 00:11.0 resource base 2424 size 4 align 2 gran 2 limit ffff flags 60000100 index 1c
   PCI: 00:11.0 resource base 2400 size 10 align 4 gran 4 limit ffff flags 60000100 index 20
   PCI: 00:11.0 resource base f024c000 size 400 align 10 gran 10 limit febfffff flags 60000200 index 24
   PCI: 00:12.0
   PCI: 00:12.0 resource base f0248000 size 1000 align 12 gran 12 limit febfffff flags 60000200 index 10
   PCI: 00:12.1
   PCI: 00:12.2
   PCI: 00:12.2 resource base f024c400 size 100 align 8 gran 8 limit febfffff flags 60000200 index 10
   PCI: 00:13.0
   PCI: 00:13.0 resource base f0249000 size 1000 align 12 gran 12 limit febfffff flags 60000200 index 10
   PCI: 00:13.1
   PCI: 00:13.2
   PCI: 00:13.2 resource base f024c500 size 100 align 8 gran 8 limit febfffff flags 60000200 index 10
   PCI: 00:14.0 child on link 0 I2C: 00:50
    I2C: 00:50
    I2C: 00:51
   PCI: 00:14.1
   PCI: 00:14.2
   PCI: 00:14.2 resource base f0244000 size 4000 align 14 gran 14 limit febfffff flags 60000201 index 10
   PCI: 00:14.3 child on link 0 PNP: 004e.0
   PCI: 00:14.3 resource base f024c700 size 1 align 0 gran 0 limit febfffff flags 60000200 index a0
   PCI: 00:14.3 resource base 0 size 1000 align 0 gran 0 limit 0 flags c0040100 index 10000000
   PCI: 00:14.3 resource base ff800000 size 800000 align 0 gran 0 limit 0 flags c0040200 index 10000100
   PCI: 00:14.3 resource base fec00000 size 1000 align 0 gran 0 limit 0 flags c0000200 index 3
    PNP: 004e.0
    PNP: 004e.0 resource base 3f0 size 8 align 3 gran 3 limit 7ff flags c0000100 index 60
    PNP: 004e.0 resource base 6 size 1 align 0 gran 0 limit 0 flags c0000400 index 70
    PNP: 004e.0 resource base 2 size 1 align 0 gran 0 limit 0 flags c0000800 index 74
    PNP: 004e.3
    PNP: 004e.3 resource base 0 size 8 align 3 gran 3 limit 7ff flags 100 index 60
    PNP: 004e.3 resource base 0 size 1 align 0 gran 0 limit 0 flags 400 index 70
    PNP: 004e.3 resource base 0 size 1 align 0 gran 0 limit 0 flags 800 index 74
    PNP: 004e.4
    PNP: 004e.4 resource base 0 size 8 align 3 gran 3 limit fff flags 100 index 60
    PNP: 004e.4 resource base 0 size 1 align 0 gran 0 limit 0 flags 400 index 70
    PNP: 004e.5
    PNP: 004e.5 resource base 60 size 1 align 0 gran 0 limit ffffffff flags e0000100 index 60
    PNP: 004e.5 resource base 64 size 0 align 0 gran 0 limit 0 flags e0000100 index 62
    PNP: 004e.5 resource base 1 size 1 align 0 gran 0 limit 0 flags e0000400 index 70
    PNP: 004e.5 resource base 0 size 1 align 0 gran 0 limit 0 flags 400 index 72
    PNP: 004e.6
    PNP: 004e.6 resource base 0 size 1 align 0 gran 0 limit 0 flags 400 index 70
    PNP: 004e.a
    PNP: 004e.10
    PNP: 004e.10 resource base 3f8 size 8 align 3 gran 3 limit 7ff flags e0000100 index 60
    PNP: 004e.10 resource base 4 size 1 align 0 gran 0 limit 0 flags e0000400 index 70
    PNP: 004e.11
    PNP: 004e.11 resource base 2f8 size 8 align 3 gran 3 limit 7ff flags c0000100 index 60
    PNP: 004e.11 resource base 3 size 1 align 0 gran 0 limit 0 flags c0000400 index 70
   PCI: 00:14.4
   PCI: 00:14.4 resource base ffff size 0 align 12 gran 12 limit ffff flags 60080102 index 1c
   PCI: 00:14.4 resource base febfffff size 0 align 20 gran 20 limit febfffff flags 60081202 index 24
   PCI: 00:14.4 resource base febfffff size 0 align 20 gran 20 limit febfffff flags 60080202 index 20
   PCI: 00:14.5
   PCI: 00:14.5 resource base f024a000 size 1000 align 12 gran 12 limit febfffff flags 60000200 index 10
   PCI: 00:15.0
   PCI: 00:15.1
   PCI: 00:15.2
   PCI: 00:15.3
   PCI: 00:16.0
   PCI: 00:16.0 resource base f024b000 size 1000 align 12 gran 12 limit febfffff flags 60000200 index 10
   PCI: 00:16.2
   PCI: 00:16.2 resource base f024c600 size 100 align 8 gran 8 limit febfffff flags 60000200 index 10
   PCI: 00:18.0
   PCI: 00:18.1
   PCI: 00:18.2
   PCI: 00:18.3
   PCI: 00:18.4
   PCI: 00:18.5
   PCI: 00:18.6
   PCI: 00:18.7
Done allocating resources.
Enabling resources...

Fam14h - domain_enable_resources: AmdInitMid.
  ader - leaving domain_enable_resources.
PCI: 00:00.0 cmd <- 06
PCI: 00:01.0 subsystem <- 1022/1510
PCI: 00:01.0 cmd <- 07
PCI: 00:01.1 subsystem <- 1022/1510
PCI: 00:01.1 cmd <- 02
PCI: 00:04.0 bridge ctrl <- 0003
PCI: 00:04.0 cmd <- 07
PCI: 00:11.0 cmd <- 03
PCI: 00:12.0 cmd <- 02
PCI: 00:12.2 cmd <- 02
PCI: 00:13.0 cmd <- 02
PCI: 00:13.2 cmd <- 02
PCI: 00:14.0 subsystem <- 1022/1510
PCI: 00:14.0 cmd <- 403
PCI: 00:14.2 cmd <- 02
PCI: 00:14.3 cmd <- 0f
PCI: 00:14.4 bridge ctrl <- 0003
PCI: 00:14.4 cmd <- 21
PCI: 00:14.5 cmd <- 02
PCI: 00:16.0 cmd <- 02
PCI: 00:16.2 cmd <- 02
PCI: 00:18.0 subsystem <- 1022/1510
PCI: 00:18.0 cmd <- 00
PCI: 00:18.1 subsystem <- 1022/1510
PCI: 00:18.1 cmd <- 00
PCI: 00:18.2 subsystem <- 1022/1510
PCI: 00:18.2 cmd <- 00
PCI: 00:18.3 subsystem <- 1022/1510
PCI: 00:18.3 cmd <- 00
PCI: 00:18.4 subsystem <- 1022/1510
PCI: 00:18.4 cmd <- 00
PCI: 00:18.5 subsystem <- 1022/1510
PCI: 00:18.5 cmd <- 00
PCI: 00:18.6 subsystem <- 1022/1510
PCI: 00:18.6 cmd <- 00
PCI: 00:18.7 subsystem <- 1022/1510
PCI: 00:18.7 cmd <- 00
PCI: 01:00.0 cmd <- 03
done.
Initializing devices...
Root Device init
APIC_CLUSTER: 0 init
start_eip=0x00002000, offset=0x00210000, code_size=0x0000005b
Initializing CPU #0
CPU: vendor AMD device 500f10
CPU: family 14, model 01, stepping 00
Model 14 Init.
Setting up local apic... apic_id: 0x00 done.
siblings = 01, CPU #0 initialized
All AP CPUs stopped
PCI: 00:00.0 init
Northbridge init
PCI: 00:01.0 init
PCI: 00:01.1 init
PCI: 00:11.0 init
PCI: 00:12.0 init
PCI: 00:12.2 init
PCI: 00:13.0 init
PCI: 00:13.2 init
PCI: 00:14.0 init
PCI: 00:14.2 init
PCI: 00:14.3 init
PCI: 00:14.4 init
PCI: 00:14.5 init
PCI: 00:16.0 init
PCI: 00:16.2 init
PCI: 00:18.0 init
PCI: 00:18.1 init
PCI: 00:18.2 init
PCI: 00:18.3 init
PCI: 00:18.4 init
PCI: 00:18.5 init
PCI: 00:18.6 init
PCI: 00:18.7 init
PCI: 01:00.0 init
PNP: 004e.5 init
PNP: 004e.10 init
Devices initialized
Show all devs...After init.
Root Device: enabled 1
APIC_CLUSTER: 0: enabled 1
APIC: 00: enabled 1
PCI_DOMAIN: 0000: enabled 1
PCI: 00:00.0: enabled 1
PCI: 00:01.0: enabled 1
PCI: 00:01.1: enabled 1
PCI: 00:04.0: enabled 1
PCI: 00:05.0: enabled 0
PCI: 00:06.0: enabled 0
PCI: 00:07.0: enabled 0
PCI: 00:08.0: enabled 0
PCI: 00:11.0: enabled 1
PCI: 00:12.0: enabled 1
PCI: 00:12.1: enabled 0
PCI: 00:12.2: enabled 1
PCI: 00:13.0: enabled 1
PCI: 00:13.1: enabled 0
PCI: 00:13.2: enabled 1
PCI: 00:14.0: enabled 1
I2C: 00:50: enabled 1
I2C: 00:51: enabled 1
PCI: 00:14.1: enabled 0
PCI: 00:14.2: enabled 1
PCI: 00:14.3: enabled 1
PNP: 004e.0: enabled 0
PNP: 004e.3: enabled 0
PNP: 004e.4: enabled 0
PNP: 004e.5: enabled 1
PNP: 004e.6: enabled 0
PNP: 004e.a: enabled 0
PNP: 004e.10: enabled 1
PNP: 004e.11: enabled 0
PCI: 00:14.4: enabled 1
PCI: 00:14.5: enabled 1
PCI: 00:15.0: enabled 0
PCI: 00:15.1: enabled 0
PCI: 00:15.2: enabled 0
PCI: 00:15.3: enabled 0
PCI: 00:18.0: enabled 1
PCI: 00:18.1: enabled 1
PCI: 00:18.2: enabled 1
PCI: 00:18.3: enabled 1
PCI: 00:18.4: enabled 1
PCI: 00:18.5: enabled 1
PCI: 00:18.6: enabled 1
PCI: 00:18.7: enabled 1
PCI: 00:16.0: enabled 1
PCI: 00:16.2: enabled 1
PCI: 01:00.0: enabled 1
APIC: 01: enabled 1
Initializing CBMEM area to 0x66ff0000 (65536 bytes)
Adding CBMEM entry as no. 1
Moving GDT to 66ff0200...ok
High Tables Base is 66ff0000.
Writing IRQ routing tables to 0xf0000...write_pirq_routing_table done.
Adding CBMEM entry as no. 2
Writing IRQ routing tables to 0x66ff0400...write_pirq_routing_table done.
PIRQ table: 48 bytes.
Wrote the mp table end at: 000f0410 - 000f0514
Adding CBMEM entry as no. 3
Wrote the mp table end at: 66ff1410 - 66ff1514
MP table: 276 bytes.
Adding CBMEM entry as no. 4
ACPI: Writing ACPI tables at 66ff2400...
ACPI:    * DSDT at 66ff24c8
ACPI:    * DSDT @ 66ff24c8 Length 27ba
ACPI: * FACS at 66ff4c88
ACPI:    * FADT at 66ff4cc8
pm_base: 0x0800
ACPI: added table 1/32, length now 40
ACPI:    * HPET at 66ff4dc0
ACPI: added table 2/32, length now 44
ACPI:    * MADT at 66ff4df8
ACPI: added table 3/32, length now 48
ACPI:    * SRAT at 66ff4e58
ACPI:   * SLIT at 66ff4e58
ACPI:    * SSDT at 66ff4e60
ACPI: added table 4/32, length now 52
ACPI:    * SSDT for PState at 66ff5495
ACPI: done.
ACPI tables: 12437 bytes.
Adding CBMEM entry as no. 5
Writing high table forward entry at 0x00000500
Wrote coreboot table at: 00000500 - 00000518  checksum b8de
New low_table_end: 0x00000518
Now going to write high coreboot table at 0x66ffe000
rom_table_end = 0x66ffe000
Adjust low_table_end from 0x00000518 to 0x00001000
Adjust rom_table_end from 0x66ffe000 to 0x67000000
Adding high table area
uma_memory_start=0x67000000, uma_memory_size=0x18000000
coreboot memory table:
 0. 0000000000000000-0000000000000fff: CONFIGURATION TABLES
 1. 0000000000001000-000000000009ffff: RAM
 2. 00000000000c0000-0000000066feffff: RAM
 3. 0000000066ff0000-0000000066ffffff: CONFIGURATION TABLES
 4. 0000000067000000-000000007effffff: RESERVED
 5. 00000000f8000000-00000000f8ffffff: RESERVED
Wrote coreboot table at: 66ffe000 - 66ffe1d8  checksum d287
coreboot table: 472 bytes.
Multiboot Information structure has been written.
 0. FREE SPACE 67000000 00000000
 1. GDT        66ff0200 00000200
 2. IRQ TABLE  66ff0400 00001000
 3. SMP TABLE  66ff1400 00001000
 4. ACPI       66ff2400 0000bc00
 5. COREBOOT   66ffe000 00002000
Check CBFS header at fffffcce
magic is 4f524243
Found CBFS header at fffffcce
Check cmos_layout.bin
CBFS: follow chain: ffc00000 + 28 + 6f0 + align -> ffc00740
Check pci1002,9802.rom
CBFS: follow chain: ffc00740 + 38 + e200 + align -> ffc0e980
Check fallback/romstage
CBFS: follow chain: ffc0e980 + 38 + 45fdc + align -> ffc549c0
Check fallback/coreboot_ram
CBFS: follow chain: ffc549c0 + 38 + 27562 + align -> ffc7bf80
Check fallback/payload
Got a payload
Loading segment from rom address 0xffc7bfb8
  data (compression=1)
  New segment dstaddr 0xf19bc memsize 0xe644 srcaddr 0xffc7bff0 filesize 0x781d
  (cleaned up) New segment addr 0xf19bc size 0xe644 offset 0xffc7bff0 filesize 0x781d
Loading segment from rom address 0xffc7bfd4
  Entry Point 0x000fcacf
Loading Segment: addr: 0x00000000000f19bc memsz: 0x000000000000e644 filesz: 0x000000000000781d
lb: [0x0000000000200000, 0x0000000000340000)
Post relocation: addr: 0x00000000000f19bc memsz: 0x000000000000e644 filesz: 0x000000000000781d
using LZMA
[ 0x000f19bc, 00100000, 0x00100000) <- ffc7bff0
dest 000f19bc, end 00100000, bouncebuffer 66d70000
Loaded segments
Jumping to boot code at fcacf
entry    = 0x000fcacf
lb_start = 0x00200000
lb_size  = 0x00140000
adjust   = 0x66cb0000
buffer   = 0x66d70000
     elf_boot_notes = 0x0024afa4
adjusted_boot_notes = 0x66efafa4
