chip northbridge/amd/gx2
  device lapic_cluster 0 on
    chip cpu/amd/model_gx2
      device lapic 0 on end
    end
  end

  #register "irqmap" = "0xaa5b"
  device pci_domain 0 on
    device pci 0.0 on end
      chip southbridge/amd/cs5535
  	register "setupflash" = "0"
        device pci 12.0 on
        device pci 12.1 off end		# SMI
        device pci 12.2 on  end		# IDE
        device pci 12.3 off end 	# Audio
        device pci 12.4 off end		# VGA
      end
    end
  end
end

