chip northbridge/via/cx700
	device lapic_cluster 0 on
		chip cpu/via/model_c7
			device lapic 0 on end
		end
	end
	device pci_domain 0 on
		device pci 0.0 on end # AGP Bridge
		device pci 0.1 on end # Error Reporting
		device pci 0.2 on end # Host Bus Control
		device pci 0.3 on end # Memory Controller
		device pci 0.4 on end # Power Management
		device pci 0.7 on end # V-Link Controller
		device pci 1.0 on     # PCI Bridge
			device pci 0.0 on end # Onboard Video
		end # PCI Bridge
		device pci f.0 on end # IDE/SATA
		#device pci f.1 on end # IDE
		device pci 10.0 on end # USB 1.1
		device pci 10.1 on end # USB 1.1
		device pci 10.2 on end # USB 1.1
		device pci 10.4 on end # USB 2.0
		device pci 11.0 on      # Southbridge LPC
			chip superio/via/vt1211
				device pnp 2e.0 on	# Floppy
					io 0x60 = 0x3f0
					irq 0x70 = 6
					drq 0x74 = 2
				end
				device pnp 2e.1 on	# Parallel Port
					io 0x60 = 0x378
					irq 0x70 = 7
					drq 0x74 = 3
				end
				device pnp 2e.2 on	# COM1
					io 0x60 = 0x3f8
					irq 0x70 = 4
				end
				device pnp 2e.3 on	# COM2
					io 0x60 = 0x2f8
					irq 0x70 = 3
				end
				device pnp 2e.b on	# HWM
					io 0x60 = 0xec00
				end
			end # superio
		end # pci 11.0
		# 1-4 non existant
		#device pci 11.5 on end # AC97 Audio
		#device pci 11.6 off end # AC97 Modem
		#device pci 12.0 on end  # Ethernet
	end # pci domain 0
end # cx700

