chip northbridge/amd/amdk8/root_complex
	device lapic_cluster 0 on
		chip cpu/amd/socket_940
			device lapic 0 on end
		end
	end
	device pci_domain 0 on
		chip northbridge/amd/amdk8
			device pci 18.0 on #  northbridge
				#  devices on link 0, link 0 == LDT 0
				chip southbridge/amd/amd8131
					# the on/off keyword is mandatory
					device pci 0.0 on end
					device pci 0.1 on end
					device pci 1.0 on end
					device pci 1.1 on end
				end
				chip southbridge/amd/amd8111
					# this "device pci 0.0" is the parent the next one
					# PCI bridge
					device pci 0.0 on
						device pci 0.0 on end
						device pci 0.1 on end
						device pci 0.2 on end
						device pci 1.0 off end
					end
					device pci 1.0 on
						chip superio/winbond/w83627thf
							device pnp 2e.0 on end
							device pnp 2e.1 on end
							device pnp 2e.2 on end
							device pnp 2e.3 on end
							device pnp 2e.4 on end
							device pnp 2e.5 on end
							device pnp 2e.6 on end
							device pnp 2e.7 on end
							device pnp 2e.8 on end
							device pnp 2e.9 on end
							device pnp 2e.a on end
						end
					end
					device pci 1.1 on end
					device pci 1.2 on end
					device pci 1.3 on end
					device pci 1.5 off end
					device pci 1.6 off end
				end
			end # LDT0
			device pci 18.0 on end # LDT1
			device pci 18.0 on end # LDT2
			device pci 18.1 on end
			device pci 18.2 on end
			device pci 18.3 on end
		end
	end
end

