chip northbridge/amd/amdk8/root_complex
	device lapic_cluster 0 on
		chip cpu/amd/socket_940
			device lapic 0 on end
		end
	end

	device pci_domain 0 on
		chip northbridge/amd/amdk8
			device pci 18.0 on end # LDT 0
			device pci 18.0 on     # LDT 1
				chip southbridge/amd/amd8131
					device pci 0.0 on end
					device pci 0.1 on end
					device pci 1.0 on end
					device pci 1.1 on end
				end
				chip southbridge/amd/amd8111
					device pci 0.0 on
						device pci 0.0 on end
						device pci 0.1 on end
						device pci 0.2 on end
						device pci 1.0 off end
                                               device pci 5.0 on end # ATI Rage XL
					end
					device pci 1.0 on
						chip superio/nsc/pc87366
							device	pnp 2e.0 off  # Floppy
								 io 0x60 = 0x3f0
								irq 0x70 = 6
								drq 0x74 = 2
							end
							device pnp 2e.1 off  # Parallel Port
								 io 0x60 = 0x378
								irq 0x70 = 7
							end
							device pnp 2e.2 off # Com 2
								 io 0x60 = 0x2f8
								irq 0x70 = 3
							end
							device pnp 2e.3 on  # Com 1
								 io 0x60 = 0x3f8
								irq 0x70 = 4
							end
							device pnp 2e.4 off end # SWC
							device pnp 2e.5 off end # Mouse
							device pnp 2e.6 on  # Keyboard
								 io 0x60 = 0x60
								 io 0x62 = 0x64
								irq 0x70 = 1
							end
							device pnp 2e.7 off end # GPIO
							device pnp 2e.8 off end # ACB
							device pnp 2e.9 off end # FSCM
							device pnp 2e.a off end # WDT
						end
					end
					device pci 1.1 on end
					device pci 1.2 on end
					device pci 1.3 on end
					device pci 1.5 off end
					device pci 1.6 off end
					register "ide0_enable" = "1"
					register "ide1_enable" = "1"
				end
			end #  device pci 18.0
			device pci 18.0 on end # LDT2
			device pci 18.1 on end
			device pci 18.2 on end
			device pci 18.3 on end
		end
	end
end

