chip northbridge/amd/gx1
  device pci_domain 0 on
    device pci 0.0 on end
      chip southbridge/amd/cs5530
        device pci 12.0 on
          chip superio/nsc/pc97317
            device pnp 2e.0 on		# Keyboard
               io 0x60 = 0x60
               io 0x62 = 0x64
              irq 0x70 = 1
            end
            device pnp 2e.1 on		# Mouse
              irq 0x70 = 12
            end
            device pnp 2e.2 on		# RTC
               io 0x60 = 0x70
              irq 0x70 = 8
            end
            device pnp 2e.3 off		# FDC
            end
            device pnp 2e.4 on		# Parallel Port
               io 0x60 = 0x378
              irq 0x70 = 7
            end
            device pnp 2e.5 on		# COM2
               io 0x60 = 0x2f8
              irq 0x70 = 3
            end
            device pnp 2e.6 on		# COM1
               io 0x60 = 0x3f8
              irq 0x70 = 4
            end
            device pnp 2e.7 on		# GPIO
               io 0x60 = 0xe0
            end
            device pnp 2e.8 on		# Power Management
               io 0x60 = 0xe800
            end
            register "com1" = "{115200}"
            register "com2" = "{38400}"
          end
        device pci 12.1 off end		# SMI
        device pci 12.2 on  end		# IDE
        device pci 12.3 off end 	# Audio
        device pci 12.4 off end		# VGA
      end
    end
  end

  chip cpu/amd/model_gx1
  end

end

