chip northbridge/via/vt8623

	device lapic_cluster 0 on
		chip cpu/via/model_c3
			device lapic 0 on  end
		end
	end

	device pci_domain 0 on

		device pci 0.0 on end
		device pci 1.0 on end

		chip southbridge/via/vt8235

			device pci 10.0 on end # USB 1.1
			device pci 10.1 on end # USB 1.1
			device pci 10.2 on end # USB 1.1
			device pci 10.3 on end # USB 2

			device pci 11.0 on      # Southbridge
				chip superio/via/vt1211
					device pnp 2e.0 on	# Floppy
						io 0x60 = 0x3f0
						irq 0x70 = 6
						drq 0x74 = 2
					end
					device pnp 2e.1 on	# Parallel Port
						io 0x60 = 0x378
						irq 0x70 = 7
						drq 0x74 = 3
					end
					device pnp 2e.2 on	# COM1
						io 0x60 = 0x3f8
						irq 0x70 = 4
					end
					device pnp 2e.3 on	# COM2
						io 0x60 = 0x2f8
						irq 0x70 = 3
					end
					device pnp 2e.b on	# HWM
						io 0x60 = 0xec00
					end

				end
			end

			device pci 11.1 on  end # IDE
			# 2-4 non existant?
			device pci 11.5 on  end # AC97 Audio
			device pci 11.6 off end # AC97 Modem
			device pci 12.0 on end  # Ethernet
		end
#		This is on the EPIA MII, not the M.
		chip southbridge/ricoh/rl5c476
			register "enable_cf" = "1"
			device pci 0a.0 on end
			device pci 0a.1 on end
		end
	end
end
