chip northbridge/amd/amdk8/root_complex
	device lapic_cluster 0 on
		chip cpu/amd/socket_940
			device lapic 0 on end
		end
	end

	device pci_domain 0 on
		chip northbridge/amd/amdk8
			device pci 18.0 on end # LDT 0
			device pci 18.0 on     # LDT 1
				chip southbridge/amd/amd8131
					device pci 0.0 on end
					device pci 0.1 on end
					device pci 1.0 on end
					device pci 1.1 on end
				end
				chip southbridge/amd/amd8111
					device pci 0.0 on
						device pci 0.0 on end
						device pci 0.1 on end
						device pci 0.2 on end
						device pci 1.0 on end
					end
					device pci 1.0 on
						chip superio/winbond/w83627hf
							device pnp 2e.0 on #  Floppy
                	                 			io 0x60 = 0x3f0
                	                			irq 0x70 = 6
                	                			drq 0x74 = 2
							end
                	        			device pnp 2e.1 off #  Parallel Port
                	                 			io 0x60 = 0x378
                	                			irq 0x70 = 7
							end
                	        			device pnp 2e.2 on #  Com1
                	                 			io 0x60 = 0x3f8
                	                			irq 0x70 = 4
							end
                	        			device pnp 2e.3 on #  Com2
                	                 			io 0x60 = 0x2f8
                	                			irq 0x70 = 3
							end
                	        			device pnp 2e.5 on #  Keyboard
                	                 			io 0x60 = 0x60
                	                 			io 0x62 = 0x64
                	                			irq 0x70 = 1
								irq 0x72 = 12
							end
                	        			device pnp 2e.6 off #  CIR
								io 0x60 = 0x100
							end
                	        			device pnp 2e.7 off #  GAME_MIDI_GIPO1
								io 0x60 = 0x220
								io 0x62 = 0x300
								irq 0x70 = 9
							end
                	        			device pnp 2e.8 off end #  GPIO2
                	        			device pnp 2e.9 off end #  GPIO3
                	        			device pnp 2e.a off end #  ACPI
                	        			device pnp 2e.b on #  HW Monitor
 					 			io 0x60 = 0x290
								irq 0x70 = 5
                					end
						end
					end
					device pci 1.1 on end
					device pci 1.2 on end
					device pci 1.3 on end
					device pci 1.5 on end
					device pci 1.6 on end
				end
			end # LDT1
			device pci 18.0 on end # LDT2
			device pci 18.1 on end
			device pci 18.2 on end
			device pci 18.3 on end
		end
	end
end

